{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMXF-A"]
[]
[]
[]
[]
["","","","","","2AMXF40A2V1B"]
["Dimensiuni","Unitate","","Înălțime","mm","550"]
["","","","Lățime","mm","765"]
["","","","Adâncime","mm","285"]
["Greutate","Unitate","","","kg","36"]
["Motor ventilator","Viteză","Răcire","Super scăzută","rot/min","500"]
["","","Încălzire","Super scăzută","rot/min","320"]
["Compresor","Tip","","","","Compresor swing etanşat ermetic"]
["Gama de operare","Răcire","Ambiant","Min.","°CDB","-10"]
["","","","Max.","°CDB","46"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","46"]
["","Încălzire","","Înalt","dBA","48"]
["Agent frigorific","Tip","","","","R-32"]
["","Cantitate","","","kg","0.88"]
["","Cantitate","","","tCO2Eq","0.60"]
["","GWP","","","","675"]
["Racorduri tubulatură","Lungime tubulatură","Max.","OU - IU","m","20"]
["Racorduri ţevi","Încărcare suplimentară de agent frigorific","","","kg/m","0,02 (pentru lungimi ale tubulaturii care depăşesc 20 m)"]
["","Diferenţa de nivel","IU - OU","Max.","m","15.0"]
["","","IU - IU","Max.","m","7.5"]
["","Lungimea totală a tubulaturii","Sistem","Real","m","30"]
["Accesorii standard","Installation manual","","","","1"]
["","Drain plug","","","","1"]
["","Screw bag","","","","1"]
["Alimentare electrică","Fază","","","","1~"]
["Alimentare curent","Frecvenţă","","","Hz","50"]
["","Tensiune","","","V","220-230-240"]
["Note","","","","","(1) - Pentru o cameră"]