{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXS-H"]
[]
[]
[]
[]
["","","","","","2MXS40H3V1B","2MXS40H3V1B2","2MXS40H2V1B","2MXS50H3V1B2","2MXS50H3V1B","2MXS50H2V1B"]
["Nivelul de presiune sonoră","Încălzire","","Nom.","dBA","48","48","","50","50"]
["","Răcire","","Nom.","dBA","47","47","","48","48"]
["Accesorii standard","Manual de instalare","","","","1","1","","1","1"]
["","Pungă şuruburi","","","","1","1","","1","1"]
["","Dop de drenare","","","","1","1","","1","1"]
["Agent frigorific","Charge","","","TCO2Eq","2.5","2.5","","3.3","3.3"]
["","GWP","","","","2,087.5","2,087.5","","2,087.5","2,087.5"]
["","Cantitate","","","kg","1.20","1.20","","1.60","1.60"]
["","Tip","","","","R-410A","R-410A","","R-410A","R-410A"]
["Racorduri conducte","Diferenţa de nivel","IU - IU","Max.","m","7.5","7.5","","7.5","7.5"]
["","","IU - OU","Max.","m","15","15","","15","15"]
["","Încărcare suplimentară de agent frigorific","","","kg/m","0,02 (pentru lungimi ale tubulaturii care depăşesc 20 m)","0,02 (pentru lungimi ale tubulaturii care depăşesc 20 m)","","0,02 (pentru lungimi ale tubulaturii care depăşesc 20 m)","0,02 (pentru lungimi ale tubulaturii care depăşesc 20 m)"]
["","Lungimea totală a tubulaturii","Sistem","Real","m","30","30","","30","30"]
["Compresor","Type","","","","Compresor oscilant etanşat ermetic_","Compresor oscilant etanşat ermetic_","","Compresor oscilant etanşat ermetic_","Compresor oscilant etanşat ermetic_"]
["Dimensiuni","Unitate","","Lățime","mm","765","765","","765","765"]
["","","","Adâncime","mm","285","285","","285","285"]
["","","","Înălțime","mm","550","550","","550","550"]
["Greutate","Unitate","","","kg","38","38","","42","42"]
["Power supply","Fază","","","","1~","1~","","1~","1~"]
["","Frecvenţă","","","Hz","50","50","","50","50"]
["","Tensiune","","","V","220-240","220-240","","220-240","220-240"]
["Note","","","","","(1) - Conţine gaze fluorurate cu efect de seră","(1) - Conţine gaze fluorurate cu efect de seră","","(1) - Conţine gaze fluorurate cu efect de seră","(1) - Conţine gaze fluorurate cu efect de seră"]
["Dimensiuni","Unitate","","Înălțime","mm","","","550","","","550"]
["","","","Lățime","mm","","","765","","","765"]
["","","","Adâncime","mm","","","285","","","285"]
["Greutate","Unitate","","","kg","","","38","","","42"]
["Compresor","Type","","","","","","Compresor swing etanşat ermetic","","","Compresor swing etanşat ermetic"]
["Gama de operare","Răcire","Ambiant","Min.","°CDB","","","10","","","10"]
["","","","Max.","°CDB","","","46","","","46"]
["","Încălzire","Ambiant","Min.","°CWB","","","-15","","","-15"]
["","","","Max.","°CWB","","","15.5","","","15.5"]
["Nivelul de presiune sonoră","Răcire","","Nom.","dBA","","","47","","","48"]
["","Încălzire","","Nom.","dBA","","","48","","","50"]
["Agent frigorific","Tip","","","","","","R-410A","","","R-410A"]
["","Cantitate","","","kg","","","1.20","","","1.60"]
["","Cantitate","","","tCO2Eq","","","2.5","","","3.3"]
["","GWP","","","","","","2087.5","","","2087.5"]
["Racorduri tubulatură","Lungime tubulatură","Max.","OU - IU","m","","","20","","","20"]
["Racorduri ţevi","Încărcare suplimentară de agent frigorific","","","kg/m","","","0,02 (pentru lungimi ale tubulaturii care depăşesc 20 m)","","","0,02 (pentru lungimi ale tubulaturii care depăşesc 20 m)"]
["","Diferenţa de nivel","IU - OU","Max.","m","","","15","","","15"]
["","","IU - IU","Max.","m","","","7.5","","","7.5"]
["","Lungimea totală a tubulaturii","Sistem","Real","m","","","30","","","30"]
["Accesorii standard","Installation manual","","","","","","1","","","1"]
["","Drain plug","","","","","","1","","","1"]
["","Screw bag","","","","","","1","","","1"]
["Alimentare electrică","Fază","","","","","","1~","","","1~"]
["Alimentare curent","Frecvenţă","","","Hz","","","50","","","50"]
["","Tensiune","","","V","","","220-240","","","220-240"]
["Accesorii standard","Ansamblu reductor","","","","","","","1","1"]
["","Reducer assembly","","","","","","","","","1"]