{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-N7"]
[]
[]
[]
[]
["","","","","","3MXM40N2V1B7","3MXM52N2V1B7"]
["Dimensiuni","Unitate","","Înălțime","mm","734","734"]
["","","","Lățime","mm","974","974"]
["","","","Adâncime","mm","401","401"]
["Greutate","Unitate","","","kg","57","57"]
["Motor ventilator","Viteză","Răcire","Super scăzută","rot/min","420","420"]
["","","Încălzire","Super scăzută","rot/min","420","420"]
["Compresor","Type","","","","Compresor swing etanşat ermetic","Compresor swing etanşat ermetic"]
["Gama de operare","Răcire","Ambiant","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","46","46"]
["Nivelul de presiune sonoră","Răcire","","Nom.","dBA","46","46"]
["","Încălzire","","Nom.","dBA","47","47"]
["Agent frigorific","Tip","","","","R-32","R-32"]
["","Cantitate","","","kg","1.8","1.8"]
["","Cantitate","","","tCO2Eq","1.22","1.22"]
["","GWP","","","","675","675"]
["Racorduri tubulatură","Lungime tubulatură","Max.","OU - IU","m","25","25 (1)"]
["Racorduri ţevi","Încărcare suplimentară de agent frigorific","","","kg/m","0,02 (pentru lungimi ale tubulaturii care depăşesc 30 m)","0,02 (pentru lungimi ale tubulaturii care depăşesc 30 m)"]
["","Diferenţa de nivel","IU - OU","Max.","m","15.0","15.0"]
["","","IU - IU","Max.","m","7.5","7.5"]
["","Lungimea totală a tubulaturii","Sistem","Real","m","50","50 (2)"]
["Accesorii standard","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Alimentare electrică","Fază","","","","1~","1~"]
["Alimentare curent","Frecvenţă","","","Hz","50","50"]
["","Tensiune","","","V","220-240","220-240"]
["Note","","","","","(1) - Pentru o cameră","(1) - Pentru o cameră"]
["","","","","","(2) - Pentru combinația cu CVXM-A, FVXM-A - lungimea maximă a condfuctelor este de 30 m.","(2) - Pentru combinația cu CVXM-A, FVXM-A - lungimea maximă a condfuctelor este de 30 m."]