{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":8,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXS-K"]
[]
[]
[]
[]
["","","","","","3MXS40K3V1B","3MXS40K3V1B2","3MXS40K2V1B"]
["Nivelul de presiune sonoră","Încălzire","","Nom.","dBA","47","47"]
["","Răcire","","Nom.","dBA","46","46"]
["Accesorii standard","Manual de instalare","","","","1","1"]
["","Dop de drenare","","","","1","1"]
["Agent frigorific","Charge","","","TCO2Eq","4.2","4.2"]
["","GWP","","","","2,087.5","2,087.5"]
["","Cantitate","","","kg","2.0","2.0"]
["","Tip","","","","R-410A","R-410A"]
["Piping connections","Diferenţa de nivel","IU - IU","Max.","m","7.5","7.5"]
["","","IU - OU","Max.","m","15","15"]
["","Încărcare suplimentară de agent frigorific","","","kg/m","0,02 (pentru lungimi ale tubulaturii care depăşesc 30 m)","0,02 (pentru lungimi ale tubulaturii care depăşesc 30 m)"]
["","Lungimea totală a tubulaturii","Sistem","Real","m","50","50"]
["Compresor","Type","","","","Compresor oscilant etanşat ermetic_","Compresor oscilant etanşat ermetic_"]
["Dimensiuni","Unitate","","Lățime","mm","936","936"]
["","","","Adâncime","mm","300","300"]
["","","","Înălțime","mm","735","735"]
["Greutate","Unitate","","","kg","49","49"]
["Power supply","Phase","","","","1~","1~"]
["","Frecvenţă","","","Hz","50","50"]
["","Tensiune","","","V","230","230"]
["Note","","","","","(1) - Conţine gaze fluorurate cu efect de seră","(1) - Conţine gaze fluorurate cu efect de seră"]
["Dimensiuni","Unitate","","Înălțime","mm","","","735"]
["","","","Lățime","mm","","","936"]
["","","","Adâncime","mm","","","300"]
["Greutate","Unitate","","","kg","","","49"]
["Compresor","Type","","","","","","Compresor swing etanşat ermetic"]
["Gama de operare","Răcire","Ambiant","Min.","°CDB","","","-10"]
["","","","Max.","°CDB","","","46"]
["","Încălzire","Ambiant","Min.","°CWB","","","-15"]
["","","","Max.","°CWB","","","15.5"]
["Nivelul de presiune sonoră","Răcire","","Nom.","dBA","","","46"]
["","Încălzire","","Nom.","dBA","","","47"]
["Agent frigorific","Tip","","","","","","R-410A"]
["","Cantitate","","","kg","","","2.0"]
["","Cantitate","","","tCO2Eq","","","4.2"]
["","GWP","","","","","","2087.5"]
["Racorduri tubulatură","Lungime tubulatură","Max.","OU - IU","m","","","50"]
["Racorduri ţevi","Încărcare suplimentară de agent frigorific","","","kg/m","","","0,02 (pentru lungimi ale tubulaturii care depăşesc 30 m)"]
["","Diferenţa de nivel","IU - OU","Max.","m","","","15"]
["","","IU - IU","Max.","m","","","7.5"]
["Accesorii standard","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["Alimentare electrică","Fază","","","","","","1~"]
["Alimentare curent","Frecvenţă","","","Hz","","","50"]
["","Tensiune","","","V","","","230"]