{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXM-A8"]
[]
[]
[]
[]
["","","","","","4MXM68A2V1B8","4MXM80A2V1B8"]
["Dimensiuni","Unitate","","Înălțime","mm","734","734"]
["","","","Lățime","mm","974","974"]
["","","","Adâncime","mm","408","408"]
["Greutate","Unitate","","","kg","63","67"]
["Compresor","Tip","","","","Compresor swing etanşat ermetic","Compresor swing etanşat ermetic"]
["Gama de operare","Răcire","Ambiant","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","50","50"]
["Nivelul de presiune sonoră","Răcire","","Nom.","dBA","48","48"]
["","Încălzire","","Nom.","dBA","49","49"]
["Agent frigorific","Tip","","","","R-32","R-32"]
["","Cantitate","","","kg","2.00","2.40"]
["","Cantitate","","","tCO2Eq","1.35","1.62"]
["","GWP","","","","675","675"]
["Racorduri tubulatură","Lungime tubulatură","Max.","OU - IU","m","25 (1)","25 (1)"]
["Racorduri ţevi","Încărcare suplimentară de agent frigorific","","","kg/m","002 (pentru lungimi ale tubulaturii care depăşesc 30 m)","002 (pentru lungimi ale tubulaturii care depăşesc 30 m)"]
["","Diferenţa de nivel","IU - OU","Max.","m","15","15"]
["","","IU - IU","Max.","m","7.5","7.5"]
["","Lungimea totală a tubulaturii","Sistem","Real","m","60","70"]
["Accesorii standard","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Alimentare electrică","Fază","","","","1~","1~"]
["Alimentare curent","Frecvenţă","","","Hz","50","50"]
["","Tensiune","","","V","220-240","220-240"]
["Note","","","","","(1) - Pentru o cameră","(1) - Pentru o cameră"]
["","","","","","(2) - Pentru combinația cu CVXM-A, FVXM-A - lungimea maximă a condfuctelor este de 30 m.","(2) - Pentru combinația cu CVXM-A, FVXM-A - lungimea maximă a condfuctelor este de 30 m."]
["","","","","","(3) - Vezi desenele separate pentru domeniul de funcţionare","(3) - Vezi desenele separate pentru domeniul de funcţionare"]
["","","","","","(4) - Vezi desenele separate pentru datele electrice","(4) - Vezi desenele separate pentru datele electrice"]
["","","","","","(5) - Conţine gaze fluorurate cu efect de seră","(5) - Conţine gaze fluorurate cu efect de seră"]