{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MWXM-A9"]
[]
[]
[]
[]
["","","","","","5MWXM68A2V1B9","5MWXM90A2V1B9"]
["Dimensiuni","Unitate","","Înălțime","mm","734","734"]
["","","","Lățime","mm","1,040","1,040"]
["","","","Adâncime","mm","408","408"]
["Greutate","Unitate","","","kg","69","73"]
["Compresor","Tip","","","","Compresor swing etanşat ermetic","Compresor swing etanşat ermetic"]
["Gama de operare","Răcire","Ambiant","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","46","46"]
["Nivelul de presiune sonoră","Răcire","","Nom.","dBA","48","52"]
["","Încălzire","","Nom.","dBA","49","53"]
["Agent frigorific","Tip","","","","R-32","R-32"]
["","Cantitate","","","kg","2","2.4"]
["","Cantitate","","","tCO2Eq","1.35","1.62"]
["","GWP","","","","675","675"]
["Racorduri tubulatură","Lungime tubulatură","Max.","OU - IU","m","25 (2)","25 (3)"]
["Racorduri ţevi","Încărcare suplimentară de agent frigorific","","","kg/m","0,02 (pentru lungimi ale tubulaturii care depăşesc 30 m)","0,02 (pentru lungimi ale tubulaturii care depăşesc 30 m)"]
["","Diferenţa de nivel","IU - OU","Max.","m","15 (3)","15"]
["","","IU - IU","Max.","m","7.5 (3)","7.5 (3)"]
["","Lungimea totală a tubulaturii","Sistem","Real","m","60","75"]
["Accesorii standard","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","2","2"]
["Alimentare electrică","Fază","","","","1~","1~"]
["Alimentare curent","Frecvenţă","","","Hz","50","50"]
["","Tensiune","","","V","220-440","220-240"]
["Note","","","","","(1) - Vezi desenele separate pentru domeniul de funcţionare","(1) - Vezi desenele separate pentru domeniul de funcţionare"]
["","","","","","(2) - Pentru o cameră","(2) - Pentru o cameră"]
["","","","","","(3) - Pentru o singură cameră (pentru combinația cu FBA71/100/125 și EKHWET și CKHWS, consultați manualul de instalare)","(3) - Pentru o singură cameră (pentru combinația cu FBA71/100/125 și EKHWET și CKHWS, consultați manualul de instalare)"]
["","","","","","(4) - Conţine gaze fluorurate cu efect de seră","(4) - Conţine gaze fluorurate cu efect de seră"]