{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MXM-M"]
[]
[]
[]
[]
["","","","","","5MXM90M2V1B"]
["Ventilator","Debit de aer","Răcire","Super scăzută","m³/min","24.1"]
["","","Încălzire","Super scăzută","m³/min","24.1"]
["","","","Super scăzută","cfm","851"]
["","","Încălzire","Super scăzută","cfm","851"]
["Dimensiuni","Unitate","","Înălțime","mm","734"]
["","","","Lățime","mm","320"]
["","","","Adâncime","mm","868"]
["Greutate","Unitate","","","kg","68"]
["Compresor","Type","","","","Compresor swing etanşat ermetic"]
["Gama de operare","Răcire","Ambiant","Min.","° C termometru uscat","-10"]
["","","","Max.","° C termometru uscat","46"]
["","Încălzire","Ambiant","Min.","°CWB","-15"]
["","","","Max.","°CWB","18"]
["Nivelul de presiune sonoră","Răcire","","Nom.","dBA","52"]
["","Încălzire","","Nom.","dBA","52"]
["Agent frigorific","Tip","","","","R-32"]
["","Cantitate","","","kg","2.4"]
["","Cantitate","","","tCO2Eq","1.6"]
["","GWP","","","","675"]
["Racorduri tubulatură","Lungime tubulatură","Max.","OU - IU","m","25"]
["Racorduri ţevi","Încărcare suplimentară de agent frigorific","","","kg/m","0,02 (pentru lungimi ale tubulaturii care depăşesc 30 m)"]
["","Diferenţa de nivel","IU - OU","Max.","m","15"]
["","","IU - IU","Max.","m","7.5"]
["","Lungimea totală a tubulaturii","Sistem","Real","m","75"]
["Accesorii standard","Installation manual","","","","1"]
["","Drain cap","","","","9"]
["","Drain plug","","","","1"]
["","Reducer assembly","","","","1"]
["","Screw bag","","","","1"]
["Alimentare electrică","Fază","","","","1~"]
["Alimentare curent","Frecvenţă","","","Hz","50"]
["","Tensiune","","","V","220-240"]