{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":9,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C"]
[]
[]
[]
[]
["","","","","","ABQ71CV1","ABQ100CV1","ABQ125CV1","ABQ140CV1"]
["Accesorii standard","Manual de instalare","","","","Manual de instalare"]
["","Manual de utilizare","","","","Manual de utilizare"]
["","Şurub + şaibă","","","","Şurub + şaibă"]
["","Telecomandă fără fir","","","","Telecomandă fără fir"]
["","Grilaj capac cu blocare","","","","Grilaj capac cu blocare"]
["","Baterie","","","","Baterie"]
["Racorduri conducte","Lichid","","Dext","mm","9.52"]
["","Gaz","","Dext","mm","15.88"]
["","Drenare","","","","19.05"]
["Putere intrare","Răcire","","Nom.","kW","0.128"]
["","Încălzire","","Nom.","kW","0.128"]
["Sound power level","Răcire","","","dBA","64"]
["","Încălzire","","","dBA","64"]
["Dimensiuni","Unitate","","Lățime","mm","600"]
["","","","Adâncime","mm","1,007"]
["","","","Înălțime","mm","285"]
["Casing","Material","","","","Oţel galvanizat"]
["Greutate","Unitate","","","kg","35"]
["Ventilator","Presiune statică externă","","Ridicată","Pa","90"]
["","","","Nom.","Pa","77"]
["","","","Scăzută","Pa","64"]
["Power supply","Phase","","","","1~"]
["","Frecvenţă","","","Hz","50"]
["","Nume","","","","V1"]
["","Tensiune","","","V","220-240"]
["Putere intrare","Încălzire","","Nom.","kW","","0.109"]
["","Răcire","","Nom.","kW","","0.109"]
["Ventilator","Presiune statică externă","","Ridicată","Pa","","70","150","150"]
["","","","Scăzută","Pa","","45","111","92"]
["Carcasă","Material","","","","","Oţel galvanizat"]
["Dimensiuni","Unitate","","Înălțime","mm","","378","378","378"]
["","","","Lățime","mm","","541","1300","1500"]
["","","","Adâncime","mm","","1045","541","541"]
["Greutate","Unitate","","","kg","","44","50","56"]
["Ventilator","Debit de aer","Răcire","Înalt","m³/min","","22.7","40.5","48.7"]
["","","","Nom.","m³/min","","20.5","37","44"]
["","","","Scăzut","m³/min","","18.3","34.8","37.9"]
["","","Încălzire","Înalt","m³/min","","22.7","40.5","48.7"]
["","","","Nom.","m³/min","","20.5","37.4","43.9"]
["","","","Scăzut","m³/min","","18.3","34.8","37.9"]
["","Presiune statică externă","","Nom.","Pa","","57","128","122"]
["Nivel de putere sonoră","Răcire","","","dBA","","60","72","73"]
["","Încălzire","","","dBA","","60","72","73"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","","41","53","55"]
["","","","Nom.","dBA","","38"]
["","","","Scăzut","dBA","","36","50","50"]
["","Încălzire","","Înalt","dBA","","41","53","55"]
["","","","Nom.","dBA","","38"]
["","","","Scăzut","dBA","","36","50","50"]
["Racorduri conducte","Lichid","","Dext","mm","","9.52","9.52","9.52"]
["","Gaz","","Dext","mm","","15.88","15.9","15.9"]
["","Drenare","","","","","19.05"]
["Accesorii standard","Installation manual","","","","","Installation manual"]
["","Wireless remote control","","","","","Wireless remote control"]
["","Cover lock grill","","","","","Cover lock grill"]
["","Battery","","","","","Battery"]
["","Screw+Washer","","","","","Screw+Washer"]
["","Operation manual","","","","","Operation manual"]
["Alimentare electrică","Fază","","","","","1~"]
["Alimentare curent","Frecvenţă","","","Hz","","50"]
["","Tensiune","","","V","","220-240"]
["Capacitate de răcire","Capacitate totală","","Nom.","kW","","","12.10","13.00"]
["Capacitate de încălzire","Capacitate totală","","Nom.","kW","","","13.5","15.5"]
["Carcasă","Culoare","","","","","","Tablă din oţel galvanizat/nevopsit","Tablă din oţel galvanizat/nevopsit"]
["Ventilator","Debit de aer","Răcire","Medie","m³/min","","","37","44"]
["","","Încălzire","Medie","m³/min","","","37.4","43.9"]
["Nivel de presiune sonoră","Răcire","","Medie","dBA","","","52","53"]
["","Încălzire","","Medie","dBA","","","52","53"]
["Sisteme de control","Telecomandă cu infraroșii","","","","","","ARCWLA","ARCWLA"]