{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":11,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A / ARXM-R"]
[]
[]
[]
[]
["","","","","ADEA35A2VEB / ARXM35R5V1B","ADEA50A2VEB / ARXM50R2V1B","ADEA50A2VEB / ARXM50R5V1B","ADEA60A2VEB / ARXM60R2V1B","ADEA60A2VEB / ARXM60R5V1B","ADEA71A2VEB / ARXM71R5V1B","ADEA71A2VEB / ARXM71R2V1B"]
["Capacitate de răcire","Nom.","","kW","3.40"]
["Eficienţă nominală","Consum anual de energie","","kWh","452"]
["","EER","","","3.76"]
["","COP","","","3.97"]
["","Directiva privind clasificarea energetică","Răcire","","A"]
["","","Încălzire","","A"]
["Capacitate de încălzire","Nom.","","kW","4.00"]
["Note","","","","(1) - Vezi desenele separate pentru domeniul de funcţionare"]
["","","","","(2) - Vezi desenele separate pentru datele electrice"]
["","","","","(3) - Capacităţile nominale de răcire se bazează pe: temperatură interioară: 27 °CDB, 19 °CWB, temperatură exterioară: 35 °CDB, lungime echivalentă traseu agent frigorific: 5 m, diferenţă de nivel: 0 m."]
["","","","","(4) - Capacităţile nominale de încălzire se bazează pe: temperatură interioară: 20°C termometru uscat, temperatura exterioară: 7°C termometru uscat, 6°C termometru umed, lungime echivalentă traseu agent frigorific: 5 m, diferenţă de nivel: 0 m."]
["Capacitate de răcire","Nom.","","kW","","5.00","5.00","5.70","5.70","6.80","6.80"]
["Capacitate de încălzire","Nom.","","kW","","5.50","5.50","7.00","7.00","7.50","7.50"]
["Eficienţă nominală","EER","","","","3.27","3.27","3.43","3.43","2.95","2.95"]
["","COP","","","","3.74","3.74","3.63","3.63","3.49","3.49"]
["","Consum anual de energie","","kWh","","765","765","831","831","1153","1153"]
["","Directiva privind clasificarea energetică","Răcire","","","A","A","A","A","C","C"]
["","","Încălzire","","","A","A","A","A","B","B"]
["Răcirea spaţiului","Clasă de eficienţă energetică","","","","A+","A+","A+","A+","A","A"]
["","Capacitate","Pdesign","kW","","5.00","5.00","5.70","5.70","6.80","6.80"]
["","SEER","","","","5.65","5.65","5.74","5.74","5.35","5.35"]
["","Consum anual de energie","","kWh/a","","310","310","347","347","445","445"]
["Încălzirea spaţiului (climat temperat)","Clasă de eficienţă energetică","","","","A+","A+","A+","A+","A","A"]
["","Capacitate","Pdesign","kW","","4.40","4.40","4.60","4.60","6.00","6.00"]
["","SCOP/A","","","","4.00","4.00","4.00","4.00","3.80","3.80"]
["","Pdh Capacitate de încălzire la -10 °","","kW","","3.73","3.73","4.00","4.00","4.83","4.83"]
["","Consum anual de energie","","kWh/a","","1538","1538","1610","1610","2209","2209"]
["Domeniu de eficiență energetică","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Capacitate de răcire","Max.","","kW","","","","","","6.98","6.98"]
["Capacitate de încălzire","Max.","","kW","","","","","","7.66","7.66"]