{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":9,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AHQ-C"]
[]
[]
[]
[]
["","","","","","AHQ71CV1","AHQ100CV1","AHQ125CV1","AHQ140CV1"]
["Putere intrare","Încălzire","","Nom.","kW","0.106","0.149"]
["","Răcire","","Nom.","kW","0.106","0.149"]
["Ventilator","Presiune statică externă","","Ridicată","Pa","0","0","0","0"]
["","","","Scăzută","Pa","0","0","0","0"]
["Capacitate de răcire","Capacitate totală","","Nom.","kW","","","12.10","13.00"]
["Capacitate de încălzire","Capacitate totală","","Nom.","kW","","","13.5","15.5"]
["Carcasă","Culoare","","","","Alb","Alb","Alb","Alb"]
["","Material","","","","Oţel galvanizat","Oţel galvanizat"]
["Dimensiuni","Unitate","","Înălțime","mm","260","260","260","285"]
["","","","Lățime","mm","1320","1538","1790","1900"]
["","","","Adâncime","mm","634","634","634","680"]
["Greutate","Unitate","","","kg","38","45","65","70"]
["Ventilator","Debit de aer","Răcire","Înalt","m³/min","23.8","31.1","34.4","43.9"]
["","","","Nom.","m³/min","21.3","27.8","31","39"]
["","","","Medie","m³/min","","","31","39"]
["","","","Scăzut","m³/min","18.9","24.8","27.2","28.3"]
["","","Încălzire","Înalt","m³/min","23.8","31.1","34.4","43.9"]
["","","","Nom.","m³/min","21.3","27.8","30.6","39.1"]
["","","","Medie","m³/min","","","30.6","39.1"]
["","","","Scăzut","m³/min","18.9","24.8","27.2","28.3"]
["","Presiune statică externă","","Nom.","Pa","0","0","0","0"]
["Nivel de putere sonoră","Răcire","","","dBA","59","64","65","71"]
["","Încălzire","","","dBA","62","64","65","71"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","49","52","52","56"]
["","","","Nom.","dBA","48","47"]
["Nivel de presiune sonoră","Răcire","","Medie","dBA","","","50","53"]
["Nivelul de presiune sonoră","Răcire","","Scăzut","dBA","46","46","49","46"]
["","Încălzire","","Înalt","dBA","49","52","52","56"]
["Nivel de presiune sonoră","Încălzire","","Medie","dBA","","","50","53"]
["Nivelul de presiune sonoră","Încălzire","","Nom.","dBA","48","47"]
["","","","Scăzut","dBA","46","46","49","46"]
["Racorduri conducte","Lichid","","Dext","mm","9.52","9.52","9.52","9.52"]
["","Gaz","","Dext","mm","15.88","15.88","15.9","15.9"]
["","Drenare","","","","19.05","19.05"]
["Sisteme de control","Telecomandă cu infraroșii","","","","ARCWLA","ARCWLA","ARCWLA","ARCWLA"]
["","Telecomandă cu fir","","","","ARCWB","ARCWB"]
["Accesorii standard","Installation manual","","","","Installation manual","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","Wireless remote control"]
["","Battery","","","","Battery","Battery"]
["","Conductă de condens","","","","Drain pipe","Drain pipe"]
["","Screw for wireless remote","","","","Screw for wireless remote","Screw for wireless remote"]
["","Ferrite Core","","","","Ferrite Core","Ferrite Core"]
["","Installation manual (Ferrite Core)","","","","Installation manual (Ferrite Core)","Installation manual (Ferrite Core)"]
["","Outdoor wiring diagram","","","","Outdoor wiring diagram","Outdoor wiring diagram"]
["","Operation manual","","","","Operation manual","Operation manual"]
["","Drain hose","","","","Drain hose","Drain hose"]
["Alimentare electrică","Fază","","","","1~","1~"]
["Alimentare curent","Frecvenţă","","","Hz","50","50"]
["","Tensiune","","","V","220-240","220-240"]