{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":12,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-N9"]
[]
[]
[]
[]
["","","","","","ARXM25N2V1B9","ARXM25N5V1B9","ARXM35N5V1B9","ARXM35N2V1B9","ARXM50N2V1B9","ARXM60N2V1B9","ARXM71N2V1B9"]
["Dimensiuni","Unitate","","Înălțime","mm","550","550","550","550","734","734","734"]
["","","","Lățime","mm","765","765","765","765","870","870","870"]
["","","","Adâncime","mm","285","285","285","285","373","373","373"]
["Greutate","Unitate","","","kg","32","32","32","32","50","50.0","50.0"]
["Compresor","Type","","","","Compresor swing etanşat ermetic","Compresor swing etanşat ermetic","Compresor swing etanşat ermetic","Compresor swing etanşat ermetic","Compresor swing etanşat ermetic","Compresor swing etanşat ermetic"]
["Gama de operare","Răcire","Ambiant","Min.","° C termometru uscat","","-10","-10","","-10","-10","-10"]
["","","","Max.","° C termometru uscat","","50","50","","50","46","46"]
["","Încălzire","Ambiant","Min.","°CWB","","-21","-21","","-21","-15","-15"]
["","","","Max.","°CWB","","18","18","","18","18","18"]
["Nivelul de presiune sonoră","Răcire","","Nom.","dBA","46","46","49","49","48","48","52"]
["","Încălzire","","Nom.","dBA","47","47","49","49","49","49","52"]
["Agent frigorific","Tip","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Cantitate","","","kg","0.76","0.76","0.76","0.76","1.15","1.15","1.15"]
["","Cantitate","","","tCO2Eq","0.52","0.52","0.52","0.52","0.78","0.78","0.78"]
["","GWP","","","","675","675","675","675","675","675","675"]
["Racorduri tubulatură","Lungime tubulatură","Max.","OU - IU","m","20","20","20","20","30","30","30"]
["Racorduri ţevi","Încărcare suplimentară de agent frigorific","","","kg/m","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)","0,020 (pentru lungimi ale tubulaturii care depăşesc 10 m)","0,035 (pentru lungimi ale tubulaturii care depăşesc 10 m)"]
["","Diferenţa de nivel","IU - OU","Max.","m","15","15","15","15","20","20","20"]
["Accesorii standard","Installation manual","","","","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1"]
["","Drain plug","","","","1","1","1","1","1","1","1"]
["Alimentare electrică","Fază","","","","1~","1~","1~","1~","1~","1~","1~"]
["Alimentare curent","Frecvenţă","","","Hz","50","50","50","50","50","50","50"]
["","Tensiune","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Accesorii standard","Drain cap","","","","","","","","3","3","3"]
["Compresor","Tip","","","","","","","","","","Compresor swing etanşat ermetic"]