{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L3"]
[]
[]
[]
[]
["","","","","","ARXS25L3V1B","ARXS35L3V1B"]
["Nivelul de presiune sonoră","Încălzire","","Înalt","dBA","","48"]
["","","","Scăzut","dBA","","45"]
["Accesorii standard","1","","","","","550"]
["Agent frigorific","Încărcare","","","kg","","2.5"]
["","Type","","","","","1.2"]
["Ventilator","Debit de aer","Răcire","Super scăzută","m³/min","","30.1"]
["","","","Super scăzută","cfm","","1,063"]
["Motor ventilator","Viteză","Răcire","Super scăzută","rpm","","740"]
["","","Încălzire","Super scăzută","rpm","","-15"]
["Gama de operare","Încălzire","Ambiant","Min.","°CWB","","20"]
["","","","Max.","°CWB","","10"]
["Nivelul de presiune sonoră","Răcire","","Scăzut","dBA","","44"]
["","","","Înalt","dBA","","48"]
["Compresor","Type","","","","","Compresor oscilant etanşat ermetic_"]
["Dimensiuni","Unitate","","Lăţime","mm","","285"]
["","","","Depth","mm","","612"]
["","","","Înălţime","mm","","765"]
["Weight","Unitate","","","kg","","34"]
["Ventilator","Debit de aer","Încălzire","Super scăzută","cfm","","904"]
["","","","Super scăzută","m³/min","","25.6"]
["Power supply","Faze","","","","","1~"]
["","Frecvenţă","","","Hz","","50"]
["","Tensiune","","","V","","220-240"]
["Note","","","","","(1) - 220V","(1) - Conţine gaze fluorurate cu efect de seră"]
["","","","","","(2) - 230 V","(2) - 220V"]
["","","","","","(3) - 240V","(3) - 230 V"]
["","","","","","","(4) - 240V"]
["Ventilator","Debit de aer","Răcire","Super scăzută","m³/min","30.1"]
["","","Încălzire","Super scăzută","m³/min","25.6"]
["","","","Super scăzută","cfm","1063"]
["","","Încălzire","Super scăzută","cfm","904"]
["Dimensiuni","Unitate","","Înălțime","mm","550"]
["","","","Lățime","mm","765"]
["","","","Adâncime","mm","285"]
["Greutate","Unitate","","","kg","34"]
["Motor ventilator","Viteză","Răcire","Super scăzută","rpm","780"]
["","","Încălzire","Super scăzută","rpm","740"]
["Compresor","Tip","","","","Compresor swing etanşat ermetic"]
["Gama de operare","Răcire","Ambiant","Min.","°CDB","10"]
["","","","Max.","°CDB","46"]
["","Încălzire","Ambiant","Min.","°CWB","-15"]
["","","","Max.","°CWB","18"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","46"]
["","Încălzire","","Înalt","dBA","47"]
["","","","Scăzut","dBA","44"]
["Agent frigorific","Tip","","","","R-410A"]
["","Cantitate","","","kg","1.0"]
["","Cantitate","","","tCO2Eq","2.1"]
["","GWP","","","","2087.5"]
["Racorduri tubulatură","Lungime tubulatură","Max.","OU - IU","m","20"]
["Racorduri ţevi","Încărcare suplimentară de agent frigorific","","","kg/m","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)"]
["","Diferenţa de nivel","IU - OU","Max.","m","15"]
["Accesorii standard","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain plug","","","","1"]
["Alimentare electrică","Fază","","","","1~"]
["Alimentare curent","Frecvenţă","","","Hz","50"]
["","Tensiune","","","V","220-240"]