{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":87,"n_cols":11,"rows_kept":87,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-A"]
[]
[]
[]
[]
["","","","","","ATXF20A5V1B","ATXF50A2V1B","ATXF60A2V1B","ATXF71A2V1B","ATXF25A5V1B (Archived)","ATXF35A5V1B (Archived)"]
["Nivelul de presiune sonoră","Încălzire","","Înalt","dBA","40","42","44","45"]
["","","","Medie","dBA","34","38","40","41"]
["","","","Funcţionare silenţioasă","dBA","21","30","32","33"]
["","","","Scăzut","dBA","28","33","35","36"]
["","Răcire","","Medie","dBA","33","39","41","42"]
["","","","Funcţionare silenţioasă","dBA","20","31","33","34"]
["","","","Scăzut","dBA","26","34","36","37"]
["","","","Înalt","dBA","40","43","45","46"]
["Accesorii standard","Manual de instalare","","","","1","1","1","1"]
["","Manual de utilizare","","","","1","1","1","1"]
["","Telecomandă prin infraroşu","","","","1","1","1","1"]
["","Baterii uscate AAA","","","","2","2","2","2"]
["","Suport telecomandă","","","","1","1","1","1"]
["","Placă de montare","","","","1","1","1","1"]
["","Şuruburi de fixare a aparatului interior","","","","2","2","2","2"]
["Sisteme de control","Telecomandă cu fir","","","","BRC944B2, BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1"]
["Racorduri ţevi","Lichid","","Dext","mm","6.35","6.35","6.35","6.35"]
["","Gaz","","Dext","mm","9.50","12.7","12.7","12.7"]
["","Drenare","","","","18","18","18","18"]
["Putere absorbită","Răcire","","Nom.","kW","0.019","0.029","0.032","0.032"]
["","Încălzire","","Nom.","kW","0.020","0.032","0.035","0.035"]
["Sound power level","Răcire","","","dBA","55","59","60","62"]
["","Încălzire","","","dBA","55","61","62","62"]
["Dimensiuni","Unitate","","Lățime","mm","770","990","990","990"]
["","","","Adâncime","mm","225","263","263","263"]
["","","","Înălțime","mm","286","295","295","295"]
["Carcasă","Culoare","","","","Alb","Alb","Alb","Alb"]
["Greutate","Unitate","","","kg","8.50","13.5","13.5","13.5"]
["Ventilator","Debit de aer","Încălzire","Înalt","m³/min","10.3","17.3","17.9","17.9"]
["","","","Scăzut","m³/min","6.7","12.2","12.8","12.8"]
["","","","Medie","m³/min","8.6","14.8","15.8","15.8"]
["","","","Funcţionare silenţioasă","m³/min","5.3","10.7","11.3","11.3"]
["","","Răcire","Scăzut","m³/min","6.1","11.9","12.2","12.2"]
["","","","Medie","m³/min","8.1","14.4","14.8","14.8"]
["","","","Înalt","m³/min","10.1","16.8","17.3","17.3"]
["","","","Funcţionare silenţioasă","m³/min","4.4","10.5","10.7","10.7"]
["Power supply","Fază","","","","1~","1~","1~","1~"]
["","Frecvenţă","","","Hz","50","50","50","50"]
["","Nume","","","","","V1","V1","V1"]
["","Tensiune","","","V","220-240","220-240","220-240","220-240"]
["Putere intrare","Răcire","","Nom.","kW","","","","","0.019","0.032"]
["","Încălzire","","Nom.","kW","","","","","0.02","0.032"]
["Carcasă","Culoare","","","","","","","","Alb","Alb"]
["Dimensiuni","Unitate","","Înălțime","mm","","","","","286","286"]
["","","","Lățime","mm","","","","","770","770"]
["","","","Adâncime","mm","","","","","225","225"]
["Greutate","Unitate","","","kg","","","","","8.5","9"]
["Ventilator","Debit de aer","Răcire","Înalt","m³/min","","","","","10.1","11.5"]
["","","","Medie","m³/min","","","","","8.1","8.3"]
["","","","Scăzut","m³/min","","","","","6.1","6.3"]
["","","","Funcţionare silenţioasă","m³/min","","","","","4.4","4.5"]
["","","Încălzire","Înalt","m³/min","","","","","10.3","11.5"]
["","","","Medie","m³/min","","","","","8.6","9"]
["","","","Scăzut","m³/min","","","","","6.7","7"]
["","","","Funcţionare silenţioasă","m³/min","","","","","5.3","5.3"]
["Nivel de putere sonoră","Răcire","","","dBA","","","","","55","58"]
["","Încălzire","","","dBA","","","","","55","58"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","","","","","40","43"]
["Nivel de presiune sonoră","Răcire","","Medie","dBA","","","","","33","34"]
["Nivelul de presiune sonoră","Răcire","","Scăzut","dBA","","","","","26","27"]
["","","","Funcţionare silenţioasă","dBA","","","","","20","20"]
["","Încălzire","","Înalt","dBA","","","","","40","40"]
["Nivel de presiune sonoră","Încălzire","","Medie","dBA","","","","","34","35"]
["Nivelul de presiune sonoră","Încălzire","","Scăzut","dBA","","","","","28","29"]
["","","","Funcţionare silenţioasă","dBA","","","","","21","21"]
["Racorduri conducte","Lichid","","Dext","mm","","","","","6.35","6.35"]
["","Gaz","","Dext","mm","","","","","9.5","9.5"]
["","Drenare","","","","","","","","18","18"]
["Sisteme de control","Telecomandă cu infraroșii","","","","","","","","ARC470A1","ARC470A1"]
["","Telecomandă cu fir","","","","","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Accesorii standard","Installation manual","","","","","","","","1","1"]
["","AAA dry-cell batteries","","","","","","","","2","2"]
["","Operation manual","","","","","","","","1","1"]
["","Indoor unit fixing screws","","","","","","","","2","2"]
["","Infrared remote control","","","","","","","","1","1"]
["","Mounting plate","","","","","","","","1","1"]
["","Remote control holder","","","","","","","","1","1"]
["Alimentare electrică","Fază","","","","","","","","1~","1~"]
["Alimentare curent","Frecvenţă","","","Hz","","","","","50","50"]
["","Tensiune","","","V","","","","","220-240","220-240"]