{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":80,"n_cols":9,"rows_kept":80,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-C"]
[]
[]
[]
[]
["","","","","","ATXF20C5V1B","ATXF25C5V1B","ATXF42C5V1B","ATXF35C5V1B (Archived)"]
["Nivelul de presiune sonoră","Încălzire","","Înalt","dBA","39.0","40.0","44.0"]
["","","","Medie","dBA","34.0","34.0","34.0"]
["","","","Funcţionare silenţioasă","dBA","21.0","21.0","22.0"]
["","","","Scăzut","dBA","28.0","28.0","28.0"]
["","Răcire","","Medie","dBA","33.0","33.0","36.0"]
["","","","Funcţionare silenţioasă","dBA","20.0","20.0","22.0"]
["","","","Scăzut","dBA","25.0","26.0","30.0"]
["","","","Înalt","dBA","39.0","40.0","45.0"]
["Accesorii standard","Manual de instalare","","","","1","1","1"]
["","Manual de utilizare","","","","1","1","1"]
["","Baterii","","","","1","1","1"]
["","Telecomandă prin infraroşu","","","","1","1","1"]
["","Baterii uscate AAA","","","","2","2","2"]
["","Suport telecomandă","","","","1","1","1"]
["","Placă de montare","","","","1","1","1"]
["","Şuruburi de fixare a aparatului interior","","","","2","2","2"]
["Sisteme de control","Wired remote control","","","","BRC073A1","BRC073A1","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","ARC470A1","ARC470A1"]
["Racorduri ţevi","Lichid","","Dext","mm","6.35","6.35","6.35"]
["","Gaz","","Dext","mm","9.50","9.50","9.50"]
["","Drenare","","","","18","18","18"]
["Putere absorbită","Răcire","","Nom.","kW","0.023","0.023","0.040"]
["","Încălzire","","Nom.","kW","0.023","0.023","0.040"]
["Sound power level","Răcire","","","dBA","53.0","54.0","59.0"]
["","Încălzire","","","dBA","55.0","55.0","59.0"]
["Dimensiuni","Unitate","","Lățime","mm","770","770","770"]
["","","","Adâncime","mm","225","225","225"]
["","","","Înălțime","mm","286","286","286"]
["Carcasă","Culoare","","","","Alb","Alb","Alb"]
["Greutate","Unitate","","","kg","8.00","8.00","9.00"]
["Power supply","Fază","","","","1~","1~","1~"]
["","Frecvenţă","","","Hz","50","50","50"]
["","Tensiune","","","V","220-440","220-440","220-440"]
["Putere intrare","Răcire","","Nom.","kW","","","","0.029"]
["","Încălzire","","Nom.","kW","","","","0.029"]
["Carcasă","Culoare","","","","","","","Alb"]
["Dimensiuni","Unitate","","Înălțime","mm","","","","286"]
["","","","Lățime","mm","","","","770"]
["","","","Adâncime","mm","","","","225"]
["Greutate","Unitate","","","kg","","","","8.5"]
["Ventilator","Debit de aer","Răcire","Înalt","m³/min","","","","11.8"]
["","","","Medie","m³/min","","","","8"]
["","","","Scăzut","m³/min","","","","6.4"]
["","","","Funcţionare silenţioasă","m³/min","","","","4.4"]
["","","Încălzire","Înalt","m³/min","","","","11.9"]
["","","","Medie","m³/min","","","","8.6"]
["","","","Scăzut","m³/min","","","","6.5"]
["","","","Funcţionare silenţioasă","m³/min","","","","5.3"]
["Nivel de putere sonoră","Răcire","","","dBA","","","","54"]
["","Încălzire","","","dBA","","","","56"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","","","","43"]
["Nivel de presiune sonoră","Răcire","","Medie","dBA","","","","34"]
["Nivelul de presiune sonoră","Răcire","","Scăzut","dBA","","","","27"]
["","","","Funcţionare silenţioasă","dBA","","","","20"]
["","Încălzire","","Înalt","dBA","","","","40"]
["Nivel de presiune sonoră","Încălzire","","Medie","dBA","","","","35"]
["Nivelul de presiune sonoră","Încălzire","","Scăzut","dBA","","","","29"]
["","","","Funcţionare silenţioasă","dBA","","","","21"]
["Racorduri conducte","Lichid","","Dext","mm","","","","6.35"]
["","Gaz","","Dext","mm","","","","9.5"]
["","Drenare","","","","","","","18"]
["Sisteme de control","Telecomandă cu infraroșii","","","","","","","ARC470A1"]
["","Telecomandă cu fir","","","","","","","BRC073A1"]
["Accesorii standard","Installation manual","","","","","","","1"]
["","AAA dry-cell batteries","","","","","","","2"]
["","Operation manual","","","","","","","1"]
["","Batteries","","","","","","","1"]
["","Indoor unit fixing screws","","","","","","","2"]
["","Infrared remote control","","","","","","","1"]
["","Mounting plate","","","","","","","1"]
["","Remote control holder","","","","","","","1"]
["Alimentare electrică","Fază","","","","","","","1~"]
["Alimentare curent","Frecvenţă","","","Hz","","","","50"]
["","Tensiune","","","V","","","","220-440"]