{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":8,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXS-K / ARXS-L3"]
[]
[]
[]
[]
["","","","","ATXS25K3V1B / ARXS25L3V1B","ATXS25K2V1B / ARXS25L3V1B","ATXS35K3V1B / ARXS35L3V1B","ATXS35K2V1B / ARXS35L3V1B"]
["Capacitate de răcire","Min.","","kW","","","1.4"]
["","Max.","","kW","","","4.0"]
["","Nom.","","kW","2.5 (2)","","3.5 (2)"]
["Piping connections","Lichid","Dext","mm","6.35","","6.35"]
["","Gaz","Dext","mm","9.5","","9.5"]
["","Drenare","Dext","mm","18","","18"]
["Eficienţă nominală","Consum anual de energie","","kWh","301","","473"]
["","EER","","","4.15 (1)","","3.70 (1)"]
["","COP","","","4.52 (1)","","4.76 (1)"]
["","Directiva privind clasificarea energetică","Răcire","","A","","A"]
["","","Încălzire","","A","","A"]
["Capacitate de încălzire","Nom.","","kW","2.8 (2)","","4.00 (2)"]
["","Min.","","kW","1.3","","1.4"]
["","Max.","","kW","4.7","","5.2"]
["Note","","","","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE","","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE"]
["","","","","(2) - Eficienţă nominală: răcire la o sarcină nominală de 35°/27°, încălzire la o sarcină nominală de 7°/20°","","(2) - Eficienţă nominală: răcire la o sarcină nominală de 35°/27°, încălzire la o sarcină nominală de 7°/20°"]
["","","","","(3) - 220V","","(3) - 220V"]
["","","","","(4) - 230 V","","(4) - 230 V"]
["","","","","(5) - 240V","","(5) - 240V"]
["Outdoor unit","","","","","ARXS25L3","","ARXS35L3"]
["Capacitate de răcire","Nom.","","kW","","2.5","","3.5"]
["Capacitate de încălzire","Nom.","","kW","","2.8","","4.00"]
["Eficienţă nominală","EER","","","","4.15","","3.70"]
["","COP","","","","4.52","","4.76"]
["","Consum anual de energie","","kWh","","301","","473"]
["","Directiva privind clasificarea energetică","Răcire","","","A","","A"]
["","","Încălzire","","","A","","A"]
["Răcirea spaţiului","Clasă de eficienţă energetică","","","","A++","","A++"]
["","Capacitate","Pdesign","kW","","2.50","","3.50"]
["","SEER","","","","7.51","","7.10"]
["","Consum anual de energie","","kWh/a","","117","","173"]
["Încălzirea spaţiului (climat temperat)","Clasă de eficienţă energetică","","","","A++","","A++"]
["","Capacitate","Pdesign","kW","","2.50","","3.60"]
["","SCOP/A","","","","4.68","","4.61"]
["","Consum anual de energie","","kWh/a","","747","","1094"]