{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1E53B"]
[]
[]
[]
[]
["","","","","BRC1E53B7"]
["Ambalare","Material","","","Carton_"]
["","Greutate","","kg","0.05"]
["Temperatura din mediul ambiant","Umiditate relativă <","","%","95"]
["Dimensiuni","Unitate integrată","Lățime","mm","160"]
["","","Înălțime","mm","55"]
["","","Adâncime","mm","150"]
["","Unitate","Lățime","mm","120"]
["","","Adâncime","mm","19"]
["","","Înălțime","mm","120"]
["Carcasă","Capac butoane","","","Nu"]
["","Culoare","","","Alb crud"]
["","LED de funcţionare","Culoare","","Verde"]
["LCD","Tip","","","Punct plin (160 x 255)"]
["","Lumina de fundal","Culoare","","Alb"]
["","Dimensiuni","Lăţime","mm","68.85"]
["","","Înălţime","mm","43.2"]
["Greutate","Unitate ambalată","","kg","0.415"]
["","Unitate","","kg","0.200"]
["Sistem auxiliar pentru căderile de tensiune","","","","Da (Ceasul va continua să funcţioneze pentru o perioadă care nu va depăşi 48 de ore)"]
["Conexiuni cabluri","Lungime cablaj","Max.","m","500"]