{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":11,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CHYHBH-AV32 / 4MXM-N"]
[]
[]
[]
[]
["","","","","","CHYHBH05AAV32 / 4MXM68N2V1B","CHYHBH05AAV32 / 4MXM80N2V1B","CHYHBH08AAV32 / 4MXM80N2V1B","CHYHBH05AFV32 / 4MXM68N2V1B","CHYHBH05AFV32 / 4MXM80N2V1B","CHYHBH08AFV32 / 4MXM80N2V1B"]
["Încălzire apă caldă menajeră","Informaţii generale","","Profil de sarcină declarat","","XL","XL","XL"]
["","Climat mediu","","Clasă de eficienţă energetică pentru încălzirea apei","","A","A","A"]
["COP","","","","","3.91 (1)","4.04 (1)","4.17 (1)","3.91","4.04","4.17"]
["Încălzire a spaţiului","Ieşire de apă la 55 °C, climat temperat","Info gen.","Seasonal space heating eff. class","","A+","A+","A+"]
["","","","ηs (eficienţă sezon. a încălzirii spaţiului)","%","113.3","120.8","120.8"]
["","","","SCOP","","2.91","3.09","3.09"]
["Capacitate de încălzire","Nom.","","","kW","4.50 (1)","4.50 (1)","6.78 (1)"]
["Note","","","","","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), boiler deviat","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), boiler deviat","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), boiler deviat","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), boiler deviat","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), boiler deviat","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), boiler deviat"]
["Capacitate de încălzire","Nom.","","","kW","","","","4.5","4.5","6.78"]
["Încălzire apă caldă menajeră","Informaţii generale","","Profil de sarcină declarat","","","","","XL","XL","XL"]
["","Climat mediu","","Clasă de eficienţă energetică pentru încălzirea apei","","","","","A","A","A"]
["Încălzire a spaţiului","Ieşire de apă la 55 °C, climat temperat","Informaţii generale","SCOP","","","","","2.91","3.09","3.09"]
["","","Informaţii gen.","Clasă de eficienţă a încălzirii spaţiului","","","","","A+","A+","A+"]