{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-AT"]
[]
[]
[]
[]
["","","","","CTXA15A2V1BT"]
["Nivelul de presiune sonoră","Încălzire","Înalt","dBA","39"]
["","","Medie","dBA","32"]
["","","Funcţionare silenţioasă","dBA","21"]
["","","Scăzut","dBA","25"]
["","Răcire","Medie","dBA","32"]
["","","Funcţionare silenţioasă","dBA","21"]
["","","Scăzut","dBA","25"]
["","","Înalt","dBA","39"]
["Accesorii standard","Manual de instalare","","","1"]
["","Manual de utilizare","","","1"]
["","Filtru de aer","","","2"]
["","Telecomandă prin infraroşu","","","1"]
["","Placă de montare telecomandă","","","1"]
["","Pungă şuruburi","","","1"]
["","Capac şuruburi","","","1"]
["","Baterii uscate AAA","","","2"]
["","Măsuri generale privind siguranţa","","","1"]
["Agent frigorific","GWP","","","675.0"]
["Sisteme de control","Wired remote control","","","BRC073"]
["","Infrared remote control","","","ARC466A58"]
["Piping connections","Lichid","Dext","mm","6.35"]
["","Gaz","Dext","mm","9.50"]
["","Drenare","","","18"]
["Putere absorbită","Răcire","Nom.","kW","0.020"]
["","Încălzire","Nom.","kW","0.020"]
["Nivel de putere sonoră","Răcire","","dBA","57"]
["Dimensiuni","Unitate","Lățime","mm","798"]
["","","Adâncime","mm","189"]
["","","Înălțime","mm","295"]
["Carcasă","Colour","","","Negru"]
["Greutate","Unitate","","kg","12"]
["Power supply","Phase","","","1~"]
["","Frecvenţă","","Hz","50"]
["","Nume","","","V1"]
["","Tensiune","","V","220-240"]