{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-BT"]
[]
[]
[]
[]
["","","","","","CTXA15B2V1BT"]
["Nivelul de presiune sonoră","Încălzire","","Înalt","dBA","39"]
["","","","Medie","dBA","32"]
["","","","Funcţionare silenţioasă","dBA","21"]
["","","","Scăzut","dBA","25"]
["","Răcire","","Medie","dBA","32"]
["","","","Funcţionare silenţioasă","dBA","21"]
["","","","Scăzut","dBA","25"]
["","","","Înalt","dBA","39"]
["Accesorii standard","Manual de instalare","","","","1"]
["","Manual de utilizare","","","","1"]
["","Filtru de aer","","","","2"]
["","Telecomandă prin infraroşu","","","","1"]
["","Placă de montare telecomandă","","","","1"]
["","Pungă şuruburi","","","","1"]
["","Capac şuruburi","","","","2"]
["","Baterii uscate AAA","","","","2"]
["","Măsuri generale privind siguranţa","","","","1"]
["Agent frigorific","GWP","","","","675.0"]
["Sisteme de control","Wired remote control","","","","BRC073"]
["","Infrared remote control","","","","ARC466A58"]
["Racorduri conducte","Lichid","","Dext","mm","6.35"]
["","Gaz","","Dext","mm","9.50"]
["","Drain","","","","18"]
["Putere intrare","Răcire","","Nom.","kW","0.020"]
["","Încălzire","","Nom.","kW","0.020"]
["Sound power level","Răcire","","","dBA","57"]
["Dimensiuni","Unitate","","Lățime","mm","798"]
["","","","Adâncime","mm","189"]
["","","","Înălțime","mm","295"]
["Carcasă","Culoare","","","","Negru"]
["Greutate","Unitate","","","kg","11.5"]
["Ventilator","Debit de aer","Încălzire","Înalt","m³/min","10.9"]
["","","","Medium","m³/min","8.7"]
["","","","Scăzut","m³/min","6.4"]
["","","","Funcţionare silenţioasă","m³/min","4.5"]
["","","Răcire","Scăzut","m³/min","6.1"]
["","","","Medium","m³/min","8.2"]
["","","","Înalt","m³/min","11.0"]
["","","","Funcţionare silenţioasă","m³/min","4.6"]
["Power supply","Fază","","","","1~"]
["","Nume","","","","V1"]
["","Frecvenţă","","","Hz","50"]
["","Tensiune","","","V","220-240"]