{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":7,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-M / 2MXM-M"]
[]
[]
[]
[]
["","","","","CTXM15M2V1B / CTXM15M2V1B / 2MXM40M2V1B","CTXM15M2V1B / CTXM15M2V1B / 2MXM40M3V1B","CTXM15M2V1B / CTXM15M2V1B / 2MXM50M2V1B"]
["Capacitate de răcire","Nom.","","kW","3.00","3.0","3.00"]
["Eficienţă nominală","Annual energy consumption","","kWh","302 (0.000)","302","310"]
["","EER","","","4.97","4.97","4.84"]
["","COP","","","4.35","4.35","4.58"]
["","Directiva privind clasificarea energetică","Răcire","","A","A","A"]
["","","Încălzire","","A","A","A"]
["Capacitate de încălzire","Nom.","","kW","3.50","3.50"]
["","Min.","","kW","","","4.00"]
["Note","","","","","","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE"]
["","","","","","(1) - Capacităţile nominale de răcire se bazează pe: temp. interioară: 27°CDB, 19°CWB, temp. exterioară: 35°CDB, lungime echiv. conducte agent frigorific: 5 m, diferenţă de nivel: 0 m. Data pentru seria cu eficienţă standard"]
["","","","","","(2) - Capacităţile nominale de încălzire se bazează pe: temperatură interioară: 20°C termometru uscat, temperatura exterioară: 7°C termometru uscat, 6°C termometru umed, lungime echivalentă traseu agent frigorific: 5 m, diferenţă de nivel: 0 m."]