{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-M / 2MXM-M9"]
[]
[]
[]
[]
["","","","","CTXM15M2V1B / CTXM15M2V1B / 2MXM50M2V1B9"]
["Capacitate de răcire","Nom.","","kW","3.0"]
["Eficienţă nominală","Annual energy consumption","","kWh","310"]
["","EER","","","4.84"]
["","COP","","","4.58"]
["","Directiva privind clasificarea energetică","Răcire","","A"]
["","","Încălzire","","A"]
["Capacitate de încălzire","Min.","","kW","4.00"]
["Note","","","","(1) - Capacităţile nominale de răcire se bazează pe: temp.interioară: 27 °CDB, 19 °CWB, temperatură exterioară: 35 °CDB, lungime echivalentă traseu agent frigorific: 5 m, diferenţă de nivel: 0 m. Date pentru seria cu eficienţă standard. Se utilizează toleranţele Eurovent 2015."]
["","","","","(2) - Capacităţile nominale de încălzire se bazează pe: temperatură interioară: 20°C termometru uscat, temperatura exterioară: 7°C termometru uscat, 6°C termometru umed, lungime echivalentă traseu agent frigorific: 5 m, diferenţă de nivel: 0 m."]