{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-N / 3MXM-A9"]
[]
[]
[]
[]
["","","","","CTXM15N2V1B / CTXM15N2V1B / CTXM15N2V1B / 3MXM40A2V1B9"]
["Capacitate de răcire","Nom.","","kW","4.00"]
["Capacitate de încălzire","Nom.","","kW","4.60"]
["Eficienţă nominală","EER","","","5.18"]
["","COP","","","5.17"]
["","Consum anual de energie","","kWh","386"]
["","Directiva privind clasificarea energetică","Răcire","","A"]
["","","Încălzire","","A"]
["Răcirea spaţiului","Clasă de eficienţă energetică","","","A+++"]
["","Capacitate","Pdesign","kW","4.00"]
["","SEER","","","8.55"]
["","Consum anual de energie","","kWh/a","164"]
["Încălzirea spaţiului (climat temperat)","Clasă de eficienţă energetică","","","A++"]
["","Capacitate","Pdesign","kW","4.90"]
["","SCOP/A","","","4.65"]
["","Pdh Capacitate de încălzire la -10 °","","kW","4.00"]
["","Consum anual de energie","","kWh/a","1475"]