{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":9,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXS-K"]
[]
[]
[]
[]
["","","","","","CTXS15K2V1B","CTXS15K3V1B","CTXS35K2V1B","CTXS35K3V1B"]
["Nivelul de presiune sonoră","Încălzire","","Înalt","dBA","38","","41"]
["","","","Funcţionare silenţioasă","dBA","21","","21"]
["","","","Scăzut","dBA","28","","30"]
["","Răcire","","Funcţionare silenţioasă","dBA","21","","21"]
["","","","Scăzut","dBA","25","","28"]
["","","","Înalt","dBA","37","","42"]
["","","","Nom.","dBA","33"]
["","Răcire","","Nom.","dBA","31","","35"]
["Accesorii standard","Manual de instalare","","","","1","","1"]
["","Manual de utilizare","","","","1","","1"]
["","Telecomandă fără fir","","","","1","","1"]
["","Baterii","","","","2","","2"]
["","Suport telecomandă","","","","1","","1"]
["","Placă de montare","","","","1","","1"]
["","Şuruburi de fixare a aparatului interior","","","","2","","2"]
["","Filtru pentru purificarea aerului din apatit de titan fotocatalitic","","","","2","","2"]
["Sisteme de control","Infrared remote control","","","","ARC466A6","","ARC466A6"]
["Piping connections","Lichid","","Dext","mm","6.35","","6.35"]
["","Gaz","","Dext","mm","9.5","","9.5"]
["","Drenare","","","","18","","18"]
["Putere absorbită","Răcire","","Nom.","kW","0.040","","0.040"]
["","Încălzire","","Nom.","kW","0.040","","0.040"]
["Nivel de putere sonoră","Răcire","","","dBA","55","","59"]
["","Încălzire","","","dBA","56","","58"]
["Dimensiuni","Unitate","","Lățime","mm","780","","780"]
["","","","Adâncime","mm","215","","215"]
["","","","Înălțime","mm","289","","289"]
["Carcasă","Colour","","","","Alb","","Alb"]
["Greutate","Unitate","","","kg","8","","8"]
["Ventilator","Debit de aer","Încălzire","Înalt","m³/min","","","10.1"]
["","","","Scăzut","m³/min","","","6.3"]
["","","","Funcţionare silenţioasă","m³/min","","","4.3"]
["","","Răcire","Scăzut","m³/min","","","5.2"]
["","","","Înalt","m³/min","","","9.2"]
["","","","Funcţionare silenţioasă","m³/min","","","3.9"]
["","","","Nom.","m³/min","","","8.1"]
["","","Răcire","Nom.","m³/min","","","7.2"]
["Power supply","Phase","","","","1~","","1~"]
["","Frecvenţă","","","Hz","50","","50"]
["","Nume","","","","V1","","V1"]
["","Tensiune","","","V","220-240","","220-240"]
["Note","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Putere intrare","Răcire","","Nom.","kW","","0.04","","0.040"]
["","Încălzire","","Nom.","kW","","0.04","","0.040"]
["Carcasă","Culoare","","","","","Alb","","Alb"]
["Dimensiuni","Unitate","","Înălțime","mm","","289","","289"]
["","","","Lățime","mm","","780","","780"]
["","","","Adâncime","mm","","215","","215"]
["Greutate","Unitate","","","kg","","8","","8.00"]
["Ventilator","Debit de aer","Răcire","Înalt","m³/min","","7.9","","9.2"]
["","","","Medie","m³/min","","6.3","","7.2"]
["","","","Scăzut","m³/min","","4.7","","5.2"]
["","","","Funcţionare silenţioasă","m³/min","","3.9","","3.9"]
["","","Încălzire","Înalt","m³/min","","9","","10.1"]
["","","","Medie","m³/min","","7.5","","8.1"]
["","","","Scăzut","m³/min","","6","","6.3"]
["","","","Funcţionare silenţioasă","m³/min","","4.3","","4.3"]
["Nivel de putere sonoră","Răcire","","","dBA","","55","","59"]
["","Încălzire","","","dBA","","56","","58"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","","37","","42"]
["Nivel de presiune sonoră","Răcire","","Medie","dBA","","31","","35"]
["Nivelul de presiune sonoră","Răcire","","Scăzut","dBA","","25","","28"]
["","","","Funcţionare silenţioasă","dBA","","21","","21"]
["","Încălzire","","Înalt","dBA","","38","","41"]
["Nivel de presiune sonoră","Încălzire","","Medie","dBA","","33","","36"]
["Nivelul de presiune sonoră","Încălzire","","Scăzut","dBA","","28","","30"]
["","","","Funcţionare silenţioasă","dBA","","21","","21"]
["Racorduri conducte","Lichid","","Dext","mm","","6.35","","6.35"]
["","Gaz","","Dext","mm","","9.5","","9.50"]
["","Drenare","","","","","18","","18"]
["Sisteme de control","Infrared remote control","","","","","ARC466A6","","ARC466A6"]
["Accesorii standard","Installation manual","","","","","1","","1"]
["","Wireless remote control","","","","","1","","1"]
["","AAA dry-cell batteries","","","","","2","","2"]
["","Operation manual","","","","","1","","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2"]
["","Indoor unit fixing screws","","","","","2","","2"]
["","Mounting plate","","","","","1","","1"]
["","Remote control holder","","","","","1","","1"]
["Alimentare electrică","Nume","","","","","V1","","V1"]
["","Fază","","","","","1~","","1~"]
["Alimentare curent","Frecvenţă","","","Hz","","50","","50"]
["","Tensiune","","","V","","220-240","","220-240"]