{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CVXM-A9"]
[]
[]
[]
[]
["","","","","","CVXM20A3V1B9"]
["Putere intrare","Răcire","","Nom.","kW","0.02"]
["","Încălzire","","Nom.","kW","0.02"]
["Carcasă","Culoare","","","","Alb"]
["Dimensiuni","Unitate","","Înălțime","mm","600"]
["","","","Lățime","mm","750"]
["","","","Adâncime","mm","238"]
["Greutate","Unitate","","","kg","17"]
["Ventilator","Debit de aer","Răcire","Înalt","m³/min","8.7"]
["","","","Medie","m³/min","7"]
["","","","Scăzut","m³/min","4.9"]
["","","","Funcţionare silenţioasă","m³/min","4.1"]
["","","Încălzire","Înalt","m³/min","9.2"]
["","","","Medie","m³/min","7.2"]
["","","","Scăzut","m³/min","5.6"]
["","","","Funcţionare silenţioasă","m³/min","4.1"]
["Nivel de putere sonoră","Răcire","","","dBA","52"]
["","Încălzire","","","dBA","52"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","38"]
["Nivel de presiune sonoră","Răcire","","Medie","dBA","32"]
["Nivelul de presiune sonoră","Răcire","","Scăzut","dBA","25"]
["","","","Funcţionare silenţioasă","dBA","22"]
["","Încălzire","","Înalt","dBA","38"]
["Nivel de presiune sonoră","Încălzire","","Medie","dBA","32"]
["Nivelul de presiune sonoră","Încălzire","","Scăzut","dBA","25"]
["","","","Funcţionare silenţioasă","dBA","21"]
["Agent frigorific","GWP","","","","675"]
["Racorduri conducte","Lichid","","Dext","mm","6.4"]
["","Gaz","","Dext","mm","9.5"]
["","Drenare","","","","VP20 (I.D. 20/O.D. 26)"]
["Control systems","Infrared remote control","","","","ARC466A66"]
["Sisteme de control","Telecomandă cu fir","","","","BRC073A1"]
["Accesorii standard","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Alimentare electrică","Fază","","","","1~"]
["Alimentare curent","Frecvenţă","","","Hz","50"]
["","Tensiune","","","V","220-240"]