{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":6,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","D2CNL-A1A"]
[]
[]
[]
[]
["","","","","","D2CNL024A1AA"]
["Gaz","Consum (G20)","","Min","m³/h","0.40"]
["","","","Max","m³/h","2.50"]
["","Clasă NOx","","","","6"]
["","Nivel NOx (G20)","","","mg/kWh","42"]
["Încălzire centrală","Aport de căldură Qn (valoare calorică netă)","Nom","Min","kW","4.0"]
["","","","Max","kW","23.5"]
["","Aport de căldură Qn (valoare calorică brută)","Nom","Min","kW","4.4"]
["","","","Max","kW","26.1"]
["","Pn ieşire la 80/60°C","","Min","kW","3.8"]
["","","","Nom","kW","22.8"]
["","Pnc ieşire la 50/30°C","","Min","kW","4.4"]
["","","","Nom","kW","24.0"]
["","Ieşire la 37/30°C","","Nom","kW","4.4"]
["","Temperatură de apă","","Max","°C","100"]
["Apă caldă menajeră","Aport de căldură Qnw (valoare calorică netă)","Nom","Min","kW","4.0"]
["","","","Max","kW","25.5"]
["","Aport de căldură Qnw (valoare calorică brută)","Nom","Min","kW","4.4"]
["","","","Max","kW","28.3"]
["","Temperatură","","Max","°C","65"]
["Aer introdus","Racord","","","mm","100"]
["","Aer introdus-=-Concentric","","","","Da"]
["Gaze de ardere","Temperatură","","Max","°C","81"]
["","Racord","","","mm","60"]
["","Debit masic (G20)","","Max","kg/h","1.7"]
["Carcasă","Culoare","","","","Alb titan (Ral9003)"]
["","Material","","","","Placă din oţel galvanizat acoperită cu vopsea pulbere"]
["Dimensiuni","Unitate","Înălţime","Carcasă","mm","590"]
["","","","Lățime","mm","400"]
["","","","Adâncime","mm","256"]
["Greutate","Unitate","","Goală","kg","27"]
["","","","Totală","kg","31"]
["Încălzire apă caldă menajeră","Informaţii generale","","Profil de sarcină declarat","","XL"]
["","","","Clasă de eficienţă energetică pentru încălzirea apei","","A"]
["Încălzirea spaţiului","Informaţii generale","","Clasa de eficienţă sezonieră pentru încălzirea spaţiului","","A"]
["Domeniu de eficiență energetică","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F"]