{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":6,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCC601A51"]
[]
[]
[]
[]
["","","","","","DCC601A51."]
["Temperatura din mediul ambiant","Umiditate relativă <","","","%","85"]
["Numărul maxim de unităţi interioare conectabile:","","","","","32"]
["Putere absorbită","kW","","","","0.015 (1)"]
["Comunicaţie","DIII-NET","","Cantitate","","1"]
["","","","Observaţie","","DIII-NET (F1F2)"]
["","Ethernet","","Cantitate","","1"]
["","Bornă de intrare","Digitală","Cantitate","","4"]
["Dimensiuni","Unitate","","Lățime","mm","384"]
["","","","Adâncime","mm","92"]
["","","","Înălțime","mm","136"]
["Numărul maxim de unităţi exterioare conectabile","","","","","7"]
["Power supply","Frecvenţă","","","Hz","50/60"]
["","Tensiune","","","V","110-240 c.a."]
["Note","","","","","(1) - Include puterea absorbită a alimentării electrice WAGO, modulul CPU şi modulul I/O"]
["","","","","","(2) - Dimensiunile includ alimentarea electrică WAGO, modulul CPU, modulul I/O şi spaţiul necesar pentru diferite componente"]
["","","","","","(3) - Dimensiunile sitei opţionale sunt: înălţime: 209 mm, lăţime: 123 mm, adâncime: 8,5 mm"]