{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":11,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EAVH-UD6V7 / EPGA011-016DV7"]
[]
[]
[]
[]
["","","","","","EAVH16SU23DA6V7 / EPGA11DAV37","EAVH16SU18DA6V7 / EPGA11DAV37","EAVH16SU18DA6V7 / EPGA14DAV37","EAVH16SU23DA6V7 / EPGA14DAV37","EAVH16SU23DA6V7 / EPGA16DAV37","EAVH16SU18DA6V7 / EPGA16DAV37"]
["Încălzire apă caldă menajeră","Informaţii generale","","Profil de sarcină declarat","","XL","L","L","XL","XL","L"]
["","Climat mediu","","Clasă de eficienţă energetică pentru încălzirea apei","","A","A","A","A","A","A"]
["COP","","","","","5.15 (1), 3.88 (2)","5.15 (1), 3.88 (2)","4.99 (1), 3.65 (2)","4.99 (1), 3.65 (2)","4.78 (1), 3.71 (2)","4.78 (1), 3.71 (2)"]
["Unitate interioară","","","","","EAVH16SU23DA6V7","EAVH16SU18DA6V7","EAVH16SU18DA6V7","EAVH16SU23DA6V7","EAVH16SU23DA6V7","EAVH16SU18DA6V7"]
["Încălzire a spaţiului","Ieşire de apă la 55 °C, climat temperat","Info gen.","Seasonal space heating eff. class","","A++","A++","A++","A++","A++","A++"]
["","","","ηs (eficienţă sezon. a încălzirii spaţiului)","%","129","129","130","130","133","133"]
["","","","SCOP","","3.29","3.29","3.34","3.34","3.41","3.41"]
["Timp de încălzire de la 10°C la 50 °C","h","","","","1h02min at 7°C ambient temperature","53min at 7°C ambient temperature","53min at 7°C ambient temperature","1h02min at 7°C ambient temperature","1h02min at 7°C ambient temperature","53min at 7°C ambient temperature"]
["Capacitate de încălzire","Nom.","","","kW","11.1 (1), 11.3 (2)","11.1 (1), 11.3 (2)","14.5 (1), 14.5 (2)","14.5 (1), 14.5 (2)","16.5 (1), 15.6 (2)","16.5 (1), 15.6 (2)"]
["Putere intrare","Încălzire","","Nom.","kW","2.16 (1), 2.91 (2)","2.16 (1), 2.91 (2)","2.91 (1), 3.96 (2)","2.91 (1), 3.96 (2)","3.45 (1), 4.21 (2)","3.45 (1), 4.21 (2)"]
["","Apă caldă menajeră de la 10°C la 50 °C","","Nom.","kWh","3.08","2.67","2.67","3.08","3.08","2.67"]
["Note","","","","","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condiţia 2: Ta de răcire 35°C - LWE 7℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Condiţia 2: Ta de răcire 35°C - LWE 7℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Condiţia 2: Ta de răcire 35°C - LWE 7℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Condiţia 2: Ta de răcire 35°C - LWE 7℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Condiţia 2: Ta de răcire 35°C - LWE 7℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Condiţia 2: Ta de răcire 35°C - LWE 7℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)"]