{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":21,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBSHB-D / ERLA11-14DV3"]
[]
[]
[]
[]
["","","","","","EBSHB11P30DF / ERLA11D2V3","EBSHB11P50DF / ERLA11D2V3","EBSHB11P30DF / ERLA11DAV3","EBSHB11P50DF / ERLA11DAV3","EBSHB11P50DG / ERLA11D2V3","EBSHB11P30DG / ERLA11DAV3","EBSHB11P30DG / ERLA11D2V3","EBSHB11P50DG / ERLA11DAV3","EBSHB16P30DF / ERLA14D2V3","EBSHB16P50DF / ERLA14D2V3","EBSHB16P30DF / ERLA14DAV3","EBSHB16P50DF / ERLA14DAV3","EBSHB16P50DG / ERLA14D2V3","EBSHB16P30DG / ERLA14DAV3","EBSHB16P30DG / ERLA14D2V3","EBSHB16P50DG / ERLA14DAV3"]
["Indoor unit","","","","","EBSHB11P30DF","EBSHB11P50DF","EBSHB11P30DF","EBSHB11P50DF","EBSHB11P50DG","EBSHB11P30DG","EBSHB11P30DG","EBSHB11P50DG","EBSHB16P30DF","EBSHB16P50DF","EBSHB16P30DF","EBSHB16P50DF","EBSHB16P50DG","EBSHB16P30DG","EBSHB16P30DG","EBSHB16P50DG"]
["Capacitate de încălzire","Nom.","","","kW","10.6 (1)","10.6 (1)","10.6 (1)","10.6 (1)","10.6 (1)","10.6 (1)","10.6 (1)","10.6 (1)","12.0 (1)","12.0 (1)","12.0 (1)","12.0 (1)","12.0","12.0","12.0","12.0"]
["Putere intrare","Încălzire","","Nom.","kW","2.19 (1)","2.19 (1)","2.19 (1)","2.19 (1)","2.19 (1)","2.19 (1)","2.19 (1)","2.19 (1)","2.46 (1)","2.46 (1)","2.46 (1)","2.46 (1)","2.46 (1)","2.46 (1)","2.46 (1)","2.46 (1)"]
["COP","","","","","4.83 (1)","4.83 (1)","4.83 (1)","4.83 (1)","4.83 (1)","4.83 (1)","4.83 (1)","4.83 (1)","4.87 (1)","4.87 (1)","4.87 (1)","4.87 (1)","4.87 (1)","4.87 (1)","4.87 (1)","4.87 (1)"]
["Încălzire apă caldă menajeră","Informaţii generale","","Profil de sarcină declarat","","L","XL","L","XL","XL","L","L","XL","L","XL","L","XL","XL","L","L","XL"]
["","Climat mediu","","Clasă de eficienţă energetică pentru încălzirea apei","","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+"]
["Încălzire a spaţiului","Ieşire de apă la 55 °C, climat temperat","Informaţii generale","SCOP","","3.23","3.23","3.23","3.23","3.23","3.23","3.23","3.23","3.22","3.22","3.22","3.22","3.22","3.22","3.22","3.22"]
["","","Informaţii gen.","Clasă de eficienţă a încălzirii spaţiului","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Ieşire de apă la 35°C, climat temperat","Informaţii generale","SCOP","","4.63","4.63","4.63","4.63","4.63","4.63","4.63","4.63","4.60","4.60","4.60","4.60","4.60","4.60","4.60","4.60"]
["","Ieşire de apă la 35 °C, climat temperat","Informaţii gen.","Clasă de eficienţă a încălzirii spaţiului","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Note","","","","","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]