{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":21,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBSXB-D / ERLA11-14DW1"]
[]
[]
[]
[]
["","","","","","EBSXB11P50DG / ERLA11D2W1","EBSXB11P30DG / ERLA11DAW1","EBSXB11P30DG / ERLA11D2W1","EBSXB11P50DG / ERLA11DAW1","EBSXB11P30DF / ERLA11DAW1","EBSXB11P50DF / ERLA11DAW1","EBSXB11P30DF / ERLA11D2W1","EBSXB11P50DF / ERLA11D2W1","EBSXB16P50DG / ERLA14D2W1","EBSXB16P30DG / ERLA14DAW1","EBSXB16P30DG / ERLA14D2W1","EBSXB16P50DG / ERLA14DAW1","EBSXB16P30DF / ERLA14DAW1","EBSXB16P50DF / ERLA14DAW1","EBSXB16P30DF / ERLA14D2W1","EBSXB16P50DF / ERLA14D2W1"]
["Unitate interioară","","","","","EBSXB11P50DG","EBSXB11P30DG","EBSXB11P30DG","EBSXB11P50DG","EBSXB11P30DF","EBSXB11P50DF","EBSXB11P30DF","EBSXB11P50DF","EBSXB16P50DG","EBSXB16P30DG","EBSXB16P30DG","EBSXB16P50DG","EBSXB16P30DF","EBSXB16P50DF","EBSXB16P30DF","EBSXB16P50DF"]
["Capacitate de încălzire","Nom.","","","kW","10.6 (1)","10.6 (1)","10.6 (1)","10.6 (1)","10.6 (1)","10.6 (1)","10.6 (1)","10.6 (1)","12.0 (1)","12.0 (1)","12.0 (1)","12.0 (1)","12.0 (1)","12.0 (1)","12.0 (1)","12.0 (1)"]
["Capacitate de răcire","Nom.","","","kW","11.2 (2)","11.2 (2)","11.2 (2)","11.2 (2)","11.2 (2)","11.2 (2)","11.2 (2)","11.2 (2)","12.9 (2)","12.9 (2)","12.9 (2)","12.9 (2)","12.9 (2)","12.9 (2)","12.9 (2)","12.9 (2)"]
["Putere intrare","Încălzire","","Nom.","kW","2.19 (1)","2.19 (1)","2.19 (1)","2.19 (1)","2.19 (1)","2.19 (1)","2.19 (1)","2.19 (1)","2.46 (1)","2.46 (1)","2.46 (1)","2.46 (1)","2.46 (1)","2.46 (1)","2.46 (1)","2.46 (1)"]
["","Răcire","","Nom.","kW","3.47 (2)","3.47 (2)","3.47 (2)","3.47 (2)","3.47 (2)","3.47 (2)","3.47 (2)","3.47 (2)","4.34 (2)","4.34 (2)","4.34 (2)","4.34 (2)","4.34 (2)","4.34 (2)","4.34 (2)","4.34 (2)"]
["COP","","","","","4.83 (1)","4.83 (1)","4.83 (1)","4.83 (1)","4.83 (1)","4.83 (1)","4.83 (1)","4.83 (1)","4.87 (1)","4.87 (1)","4.87 (1)","4.87 (1)","4.87 (1)","4.87 (1)","4.87 (1)","4.87 (1)"]
["EER","","","","","3.22 (2)","3.22 (2)","3.22 (2)","3.22 (2)","3.22 (2)","3.22 (2)","3.22 (2)","3.22 (2)","2.98 (2)","2.98 (2)","2.98 (2)","2.98 (2)","2.98 (2)","2.98 (2)","2.98 (2)","2.98 (2)"]
["Încălzire apă caldă menajeră","Informaţii generale","","Profil de sarcină declarat","","XL","L","L","XL","L","XL","L","XL","XL","L","L","XL","L","XL","L","XL"]
["","Climat mediu","","Clasă de eficienţă energetică pentru încălzirea apei","","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+"]
["Încălzire a spaţiului","Ieşire de apă la 55 °C, climat temperat","Informaţii generale","SCOP","","3.27","3.27","3.27","3.27","3.27","3.27","3.27","3.27","3.26","3.26","3.26","3.26","3.26","3.26","3.26","3.26"]
["","","Informaţii gen.","Clasă de eficienţă a încălzirii spaţiului","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Ieşire de apă la 35°C, climat temperat","Informaţii generale","SCOP","","4.72","4.72","4.72","4.72","4.72","4.72","4.72","4.72","4.68","4.68","4.68","4.68","4.68","4.68","4.68","4.68"]
["","Ieşire de apă la 35 °C, climat temperat","Informaţii gen.","Clasă de eficienţă a încălzirii spaţiului","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Domeniu de eficiență energetică","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Note","","","","","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condiţia 2: Ta de răcire 35°C - LWE 7℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Condiţia 2: Ta de răcire 35°C - LWE 7℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Condiţia 2: Ta de răcire 35°C - LWE 7℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Condiţia 2: Ta de răcire 35°C - LWE 7℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Condiţia 2: Ta de răcire 35°C - LWE 7℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Condiţia 2: Ta de răcire 35°C - LWE 7℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Condiţia 2: Ta de răcire 35°C - LWE 7℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Condiţia 2: Ta de răcire 35°C - LWE 7℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Condiţia 2: Ta de răcire 35°C - LWE 7℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Condiţia 2: Ta de răcire 35°C - LWE 7℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Condiţia 2: Ta de răcire 35°C - LWE 7℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Condiţia 2: Ta de răcire 35°C - LWE 7℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Condiţia 2: Ta de răcire 35°C - LWE 7℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Condiţia 2: Ta de răcire 35°C - LWE 7℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Condiţia 2: Ta de răcire 35°C - LWE 7℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Condiţia 2: Ta de răcire 35°C - LWE 7℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)"]