{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":7,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSAH-D9W"]
[]
[]
[]
[]
["","","","","","EGSAH06DA9W","EGSAH10DA9W"]
["Capacitate de încălzire","Min.","","","kW","0.85","0.85"]
["","Nom.","","","kW","3.35","5.49"]
["","Max.","","","kW","7.98","9.55"]
["Putere intrare","Nom.","","","kW","0.74","1.17"]
["COP","","","","","4.51","4.7"]
["Carcasă","Culoare","","","","Alb + negru","Alb + negru"]
["","Material","","","","Foaie metalică prevopsită"]
["Dimensiuni","Unitate","","Înălțime","mm","1891","1891"]
["","","","Lățime","mm","597","597"]
["","","","Adâncime","mm","666","666"]
["Greutate","Unitate","","","kg","222","222"]
["Rezervor","Volum de apă","","","l","180","180"]
["","Izolaţie","","Pierderea de căldură","kWh/24 h","1.2","1.2"]
["","Protecţie anticoroziune","","","","Decapare","Decapare"]
["Agent frigorific","Tip","","","","R-32","R-32"]
["","GWP","","","","675.0","675.0"]
["","Cantitate","","","tCO2Eq","1.15","1.15"]
["","Cantitate","","","kg","1.70","1.70"]
["Încălzire a spaţiului","Ieşire de apă la 55 °C, climat temperat","Informaţii generale","SCOP","","3.72 (1)","4.00 (1)"]
["","","Informaţii gen.","Clasă de eficienţă a încălzirii spaţiului","","A++","A+++"]
["","Ieşire de apă la 35°C, climat temperat","Informaţii generale","SCOP","","5.06 (1)","5.12 (1)"]
["","Ieşire de apă la 35 °C, climat temperat","Informaţii gen.","Clasă de eficienţă a încălzirii spaţiului","","A+++","A+++"]
["Alimentare electrică","Fază","","","","1~/3~","1~/3~"]
["Alimentare curent","Frecvenţă","","","Hz","50","50"]
["","Tensiune","","","V","230/400","230/400"]
["Curent","Siguranţe recomandate","","","A","16/32","16/32"]
["Note","","","","","(1) - Conform EN14825 și EN14511:2018","(1) - Conform EN14825 și EN14511:2018"]