{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSQH-A9W"]
[]
[]
[]
[]
["","","","","","EGSQH10S18AA9W"]
["Nivelul de presiune sonoră","Nom.","","","dBA","32.0 (6)"]
["Agent frigorific","GWP","","","","2,090"]
["","Încărcare","","","kg","1.80"]
["","Tip","","","","R-410A"]
["Gama de operare","Spaţiu de instalare","","Min.","°C","5.00"]
["","","","Max.","°C","30.0"]
["","Încălzire","Partea de apă","Max.","°C","60.0 (7), 65.0 (8)"]
["","","","Min.","°C","24 (7), 24 (8)"]
["","Partea de apă sărată","","Min.","°C","-5.00"]
["","","","Max.","°C","20.0"]
["","Apă caldă menajeră","Partea de apă","Max.","°C","55 (7), 60 (9)"]
["","","","Min.","°C","25 (7), 25 (9)"]
["Putere intrare","Nom.","","","kW","2.38 (1), 2.89 (2)"]
["Nivel de putere sonoră","Nom.","","","dBA","46.0"]
["COP","","","","","4.33 (1), 3.18 (2)"]
["Dimensiuni","Unitate","","Lățime","mm","600"]
["","","","Adâncime","mm","728"]
["","","","Înălțime","mm","1,730"]
["Carcasă","Material","","","","Foaie metalică prevopsită"]
["","Culoare","","","","Alb"]
["Rezervor","Volum de apă","","","l","180"]
["","Protecţie anticoroziune","","","","Anod"]
["","Izolaţie","","Pierderea de căldură","kWh/24 h","1.36 (4)"]
["Greutate","Unitate","","","kg","210"]
["Încălzire a spaţiului","Ieşire de apă la 35°C, climat temperat","Info gen.","ηs (eficienţă sezon. a încălzirii spaţiului)","%","194"]
["","","","Clasă de eficienţă a încălzirii spaţiului","","A+++"]
["","","","SCOP","","5.06"]
["","Ieşire de apă la 55 °C, climat temperat","Info gen.","Seasonal space heating eff. class","","A++"]
["","","","ηs (eficienţă sezon. a încălzirii spaţiului)","%","139"]
["","","","SCOP","","3.68"]
["Capacitate de încălzire","Nom.","","","kW","10.3 (1), 9.20 (2)"]
["","Min.","","","kW","3.11 (1), 2.47 (2)"]
["","Max.","","","kW","13.0 (1), 11.9 (2)"]
["Power supply","Fază","","","","3~"]
["","Nume","","","","9W"]
["","Frecvenţă","","","Hz","50"]
["","Tensiune","","","V","400"]
["Curent","Siguranţe recomandate","","","A","25"]
["Note","","","","","(1) - EWB/LWB 0°C/-3°C - LWC 35°C (DT=5°C)"]
["","","","","","(2) - EWB/LWB 0°C/-3°C - LWC 45℃ (DT=5°C)"]
["","","","","","(3) - cu 40% propilenglicol"]
["","","","","","(4) - Pierdere de căldură în conformitate cu EN12897"]
["","","","","","(5) - inclusiv tubulatură + PHE + încălzitor de rezervă/fără vas de expansiune"]
["","","","","","(6) - Nivelul presiunii sonore este măsurat cu un microfon, la o distanţă de 1 m faţă de unitate. Este o valoare relativă, dependentă de distanţă şi de mediul acustic."]
["","","","","","(7) - Cu pompă de căldură"]
["","","","","","(8) - Cu pompă de căldură + încălzitor de rezervă"]
["","","","","","(9) - Cu încălzitor de rezervă"]