{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":9,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSX-D3"]
[]
[]
[]
[]
["","","","","","EHSX04P30DA3","EHSX04P50DA3","EHSX08P30DA3","EHSX08P50DA3"]
["Carcasă","Culoare","","","","Alb trafic (RAL9016)/Gri închis (RAL7011)","Alb trafic (RAL9016)/Gri închis (RAL7011)","Alb trafic (RAL9016)/Gri închis (RAL7011)","Alb trafic (RAL9016)/Gri închis (RAL7011)"]
["","Material","","","","Polipropilenă rezistentă la impact","Polipropilenă rezistentă la impact","Polipropilenă rezistentă la impact","Polipropilenă rezistentă la impact"]
["Dimensiuni","Unitate","","Înălțime","mm","1891","1896","1891","1896"]
["","","","Lățime","mm","595","790","595","790"]
["","","","Adâncime","mm","615","790","615","790"]
["Greutate","Unitate","","","kg","73.0","93.0","73.0","93.0"]
["PED","Categorie","","","","art. 3,3","art. 3,3","art. 3,3","art. 3,3"]
["Agent frigorific","Tip","","","","R-32","R-32","R-32","R-32"]
["","GWP","","","","675.0","675.0","675.0","675.0"]
["","Cantitate","","","kg","1.50","1.50","1.50","1.50"]
["Nivel de putere sonoră","Nom.","","","dBA","39","39","39","39"]
["Gama de operare","Încălzire","Partea de apă","Min.","°C","18","18","18","18"]
["","","","Max.","°C","65","65","65","65"]
["","Răcire","Ambiant","Min.","° C termometru uscat","10","10","10","10"]
["","","Partea de apă","Min.","°C","5","5","5","5"]
["","","","Max.","°C","22","22","22","22"]
["Alimentare electrică","Fază","","","","1~","1~","1~","1~"]
["Alimentare curent","Frecvenţă","","","Hz","50","50","50","50"]
["","Tensiune","","","V","230","230","230","230"]
["Încălzitor electric","Alimentare curent","","Nume","","3V / 9W","3V / 9W","3V / 9W","3V / 9W"]
["","","","Faze","","1~ / 3~","1~ / 3~","1~ / 3~","1~ / 3~"]
["","","","Frecvenţă","Hz","50","50","50","50"]
["Note","","","","","(1) - Pierdere de căldură în conformitate cu EN12897","(1) - Pierdere de căldură în conformitate cu EN12897","(1) - Pierdere de căldură în conformitate cu EN12897","(1) - Pierdere de căldură în conformitate cu EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65℃","(4) - TKW = 10°C/TWW = 40°C/TSP = 65℃","(4) - TKW = 10°C/TWW = 40°C/TSP = 65℃","(4) - TKW = 10°C/TWW = 40°C/TSP = 65℃"]
["","","","","","","(5) - Încălzirea rezervorului cu pompa de căldură, fără încălzitor electric","","(5) - Încălzirea rezervorului cu pompa de căldură, fără încălzitor electric"]