{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":9,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVX-E6V / ERGA-EVH7"]
[]
[]
[]
[]
["","","","","","EHVX08S18EA6V / ERGA08EAV3H7","EHVX08S18EJ6V / ERGA08EAV3H7","EHVX08S23EA6V / ERGA08EAV3H7","EHVX08S23EJ6V / ERGA08EAV3H7"]
["Capacitate de încălzire","Nom.","","","kW","7.5 (1), 7.8 (2)","7.5 (1), 7.8 (2)","7.5 (1), 7.8 (2)","7.5 (1), 7.8 (2)"]
["Capacitate de răcire","Nom.","","","kW","6.25 (1), 5.44 (2)","6.25 (1), 5.44 (2)","6.25 (1), 5.44 (2)","6.25 (1), 5.44 (2)"]
["Putere intrare","Încălzire","","Nom.","kW","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)"]
["","Răcire","","Nom.","kW","1.16 (1), 1.73 (2)","1.16 (1), 1.73 (2)","1.16 (1), 1.73 (2)","1.16 (1), 1.73 (2)"]
["Putere absorbită","Apă caldă menajeră de la 10°C la 50 °C","","Nom.","kWh","2.48","2.48","3.01","3.01"]
["Timp de încălzire de la 10°C la 50 °C","h","","","","1 h 28 min","1 h 28 min","1 h 40 min","1 h 40 min"]
["COP","","","","","4.6 (1), 3.5 (2)","4.6 (1), 3.5 (2)","4.6 (1), 3.5 (2)","4.6 (1), 3.5 (2)"]
["EER","","","","","5.4 (1), 3.14 (2)","5.4 (1), 3.14 (2)","5.4 (1), 3.14 (2)","5.4 (1), 3.14 (2)"]
["Încălzire apă caldă menajeră","Informaţii generale","","Profil de sarcină declarat","","L","L","XL","XL"]
["","Climat mediu","","Clasă de eficienţă energetică pentru încălzirea apei","","A+","A+","A+","A+"]
["Încălzire a spaţiului","Ieşire de apă la 55 °C, climat temperat","Informaţii generale","SCOP","","3.35","3.35","3.35","3.35"]
["","","Informaţii gen.","Clasă de eficienţă a încălzirii spaţiului","","A++","A++","A++","A++"]
["","Ieşire de apă la 35°C, climat temperat","Informaţii generale","SCOP","","4.61","4.61","4.61","4.61"]
["","Ieşire de apă la 35 °C, climat temperat","Informaţii gen.","Clasă de eficienţă a încălzirii spaţiului","","A+++","A+++","A+++","A+++"]
["Note","","","","","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condiţia 1: Ta de răcire 35°C - LWE 18℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condiţia 2: Ta de răcire 35°C - LWE 7℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Condiţia 2: Ta de răcire 35°C - LWE 7℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Condiţia 2: Ta de răcire 35°C - LWE 7℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Condiţia 2: Ta de răcire 35°C - LWE 7℃ (DT = 5°C); Ta de încălzire DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)"]