{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":6,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHH2E-AV3"]
[]
[]
[]
[]
["","","","","","EKHH2E260AAV3"]
["Sound power level","Domestic hot water heating","","Indoor unit","dBA","53"]
["","","","Unitate exterioară","dBA","52"]
["Încălzire apă caldă menajeră","Informaţii generale","","Clasă de eficienţă energetică pentru încălzirea apei","","A+"]
["","","","Setare temperatură termostat","°C","55"]
["","","","Profil de sarcină declarat","","XL"]
["","Climat rece","","CAE (consum anual de energie)","kWh","1,826"]
["","Climat cald","","CAE (consum anual de energie)","kWh","1,296"]
["","Climat mediu","","CAE (consum anual de energie)","kWh","1,323"]
["Equivalent hot water","Max","","","l","342"]
["Pompă de căldură","Pornire automată degivrare","","","°C","-2"]
["","Domeniu de funcţionare","Ambiant","Min.","°CDB","-7"]
["","","","Max.","°CDB","38"]
["","Carcasă","","Material","","Capac: Finisaj superior EPP"]
["","","","Colour","","White body / black top"]
["","Presiune sistem","","Max.","bar","7"]
["","Defrost method","","","","Activ cu ventil de gaz fierbinte"]
["COP","","","","","3.10 (1), 3.60 (2)"]
["Agent frigorific","GWP","","","","1,430.0"]
["","Încărcare","","","kg","0.900"]
["","Tip","","","","R-134a"]
["Compresor","Type","","","","Rotary non-inverter"]
["Dimensions","Unit","","Diametru","mm","650"]
["","","","Înălţime","mm","2,000"]
["Apă caldă menajeră","Ieşire","","Nom","kW","1.8"]
["Rezervor","Installation","","Solar thermal connection possible","","Nu"]
["","Integrated heating element power","","Nom.","kW","1.5"]
["","Casing","","Material","","ABS presat"]
["","","","Culoare","","Alb"]
["","Dimensiuni","Unitate","Înălţime","mm","1,500"]
["","Domeniu de funcţionare","Partea de apă","Max.","°C","56"]
["","","","Min.","°C","10"]
["Greutate","Unitate integrată","","","kg","115"]
["","Unitate","","Goală","kg","95"]
["","","","Totală","kg","349"]
["Locul de instalare","","","","","Interior"]
["IP class","","","","","IP-X4"]
["General","Product description","","Pompă de căldură aer-apă","","da"]
["","Detalii furnizor/producător","","Name and address","","ELIC - Via Pietro Zorutti 13/14, 33074 Fontanafredda ITALY"]
["Heat up time","Max.","","","hh:mm","10:14:00, 07:56:46"]
["Pompă de căldură","Alimentare curent","","Frecvenţă","Hz","50"]
["","","","Curent maxim de lucru","A","2"]
["","","","Fază","","1P"]
["","","","Tensiune","V","230"]
["Rezervor","Alimentare curent","","Fază","","1P"]
["","","","Frecvenţă","Hz","50"]
["","","","Tensiune","V","230"]
["Note","","","","","(1) - Conform EN16147-2011, temperatură de intrare 7 °C, temperatură cameră 20 °C, intrare apă rece 10 °C"]
["","","","","","(2) - Conform EN16147-2011, temperatură de intrare 15°C, temperatură cameră 20 °C, intrare apă rece 10 °C"]
["","","","","","(3) - Temperatură interioară: 29°C termometru uscat, 19°C termometru umed; temperatură exterioară: 46°C termometru uscat, 24°C termometru umed"]
["","","","","","(4) - Temperatură interioară: 27°C termometru uscat, 19°C termometru umed; temperatură exterioară: 35°C termometru uscat, 24°C termometru umed"]