{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERLA-DW17"]
[]
[]
[]
[]
["","","","","","ERLA16D2W17","ERLA16DAW17"]
["Dimensiuni","Unitate","","Înălțime","mm","870","870"]
["","","","Lățime","mm","1,100","1,100"]
["","","","Adâncime","mm","460","460"]
["Greutate","Unitate","","","kg","101","101"]
["Ventilator","Debit de aer","Încălzire","Înalt","m³/min","85.0","85.0"]
["","","Răcire","Înalt","m³/min","85","85"]
["Domeniu de funcţionare","Răcire","","Min.","° C termometru uscat","10","10"]
["","","","Max.","° C termometru uscat","43","43"]
["Gama de operare","Apă caldă menajeră","","Min.","° C termometru uscat","-25","-25"]
["Domeniu de funcţionare","Apă caldă menajeră","","Max.","° C termometru uscat","25 (1), 35 (1)","25 (1), 35 (1)"]
["Nivel de putere sonoră","Încălzire","","Nom.","dBA","62.0 (2)","62.0 (2)"]
["Nivelul de presiune sonoră","Încălzire","","Nom.","dBA","48.0 (2)","48.0 (2)"]
["Agent frigorific","Tip","","","","R-32","R-32"]
["","GWP","","","","675.0","675.0"]
["","Cantitate","","","tCO2Eq","2.57","2.57"]
["","Cantitate","","","kg","3.8","3.8"]
["Racorduri conducte","Lichid","","Dext","mm","9.5","9.5"]
["","Gaz","","Dext","mm","15.9","15.9"]
["Racorduri ţevi","Drenare","","Dext","mm","26","26"]
["","Diferenţa de nivel","IU - OU","Max.","m","30.0","30.0"]
["Racorduri conducte","Izolație termică","","","","Ţevile cu lichid şi cele cu gaz","Ţevile cu lichid şi cele cu gaz"]
["Alimentare electrică","Nume","","","","W1","W1"]
["","Fază","","","","3~","3~"]
["Alimentare curent","Frecvenţă","","","Hz","50","50"]
["","Tensiune","","","V","400","400"]
["Curent","Siguranţe recomandate","","","A","16","16"]
["Note","","","","","(1) - Pentru mai multe detalii, consultaţi desenul pentru domeniul de funcţionare","(1) - Pentru mai multe detalii, consultaţi desenul pentru domeniul de funcţionare"]
["","","","","","(2) - Măsurat la o pierdere de presiune de 10 kPa în sistemul de încălzire, în condiții de funcționare ale apei de ieșire de 47-55 °C, într-o cameră cu o temperatură ambiantă de 20 °C. DB/WB 7°C/6°.","(2) - Măsurat la o pierdere de presiune de 10 kPa în sistemul de încălzire, în condiții de funcționare ale apei de ieșire de 47-55 °C, într-o cameră cu o temperatură ambiantă de 20 °C. DB/WB 7°C/6°."]