{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSH16E"]
[]
[]
[]
[]
["","","","","","ETSH16P30EF","ETSH16P50EF"]
["Carcasă","Culoare","","","","Alb (RAL9016)/negru (RAL9017)","Alb (RAL9016)/negru (RAL9017)"]
["","Material","","","","Polipropilenă rezistentă la impact","Polipropilenă rezistentă la impact"]
["Dimensiuni","Unitate","","Înălțime","mm","1,892","1,910"]
["","","","Lățime","mm","594","792"]
["","","","Adâncime","mm","644","816"]
["Greutate","Unitate","","","kg","75","98"]
["Nivel de putere sonoră","Nom.","","","dBA","45.6","45.6"]
["Nivelul de presiune sonoră","Nom.","","","dBA","32.8","32.8"]
["Gama de operare","Încălzire","Partea de apă","Min.","°C","0 (2)","0 (2)"]
["","","","Max.","°C","0 (2)","0 (2)"]
["","Răcire","Ambiant","Min.","° C termometru uscat","0 (2)","0 (2)"]
["","","Partea de apă","Min.","°C","0 (2)","0 (2)"]
["","","","Max.","°C","0 (2)","0 (2)"]
["Power supply","Fază","","","","1~","1~"]
["","Frecvenţă","","","Hz","50","50"]
["","Tensiune","","","V","230","230"]
["Note","","","","","(1) - Pierdere de căldură în conformitate cu EN12897","(1) - Pierdere de căldură în conformitate cu EN12897"]
["","","","","","(2) - Consultați schema limitelor de funcționare","(2) - Consultați schema limitelor de funcționare"]