{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B"]
[]
[]
[]
[]
["","","","","","FAA71BUV1B","FAA100BUV1B"]
["Carcasă","Culoare","","","","Alb","Alb"]
["","Material","","","","Răşină","Răşină"]
["Dimensiuni","Unitate","","Înălțime","mm","290","340"]
["","","","Lățime","mm","1050","1200"]
["","","","Adâncime","mm","269","262"]
["Greutate","Unitate","","","kg","14","18"]
["Ventilator","Debit de aer","Răcire","Înalt","m³/min","16.2","23"]
["","","","Medie","m³/min","13.4","21.1"]
["","","","Scăzut","m³/min","12.1","18.7"]
["","","Încălzire","Înalt","m³/min","16.9","23"]
["","","","Medie","m³/min","14.2","20.9"]
["","","","Scăzut","m³/min","12.7","18.7"]
["Nivel de putere sonoră","Răcire","","","dBA","61","65"]
["","Încălzire","","","dBA","61","65"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","45","49"]
["Nivel de presiune sonoră","Răcire","","Medie","dBA","42","45"]
["Nivelul de presiune sonoră","Răcire","","Scăzut","dBA","40","41"]
["","Încălzire","","Înalt","dBA","45","49"]
["Nivel de presiune sonoră","Încălzire","","Medie","dBA","42","45"]
["Nivelul de presiune sonoră","Încălzire","","Scăzut","dBA","40","41"]
["Racorduri conducte","Lichid","","Dext","mm","9.52","9.52"]
["","Gaz","","Dext","mm","15.9","15.9"]
["","Drenare","","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Alimentare electrică","Fază","","","","1~","1~"]
["Alimentare curent","Frecvenţă","","","Hz","50","50"]
["","Tensiune","","","V","220-240","220-240"]
["Accesorii standard","Installation plate","","","","1","1"]
["","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","4","4"]
["","Heat insulating tape","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["","Screw bag","","","","1","1"]
["Note","","","","","(1) - Capacităţile nom. de răcire se bazează pe: temperatură interioară: 27 °CDB, 19 °CWB, temperatură exterioară: 35 °CDB, lungime echivalentă traseu agent frigorific: 5 m, diferenţă de nivel: 0 m."]
["","","","","","(2) - Capacităţile nominale de încălzire se bazează pe: temperatură interioară: 20°C termometru uscat, temperatura exterioară: 7°C termometru uscat, 6°C termometru umed, lungime echivalentă traseu agent frigorific: 5 m, diferenţă de nivel: 0 m."]
["Accesorii standard","Screw cover","","","","","3"]