{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":9,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FAQ100CVEB / RZQG71L9V1B","FAQ71CVEB / RZQG71L9V1B","FAQ71CVEB / FAQ71CVEB / RZQG100L9V1B","FAQ100CVEB / RZQG100L9V1B","FAQ71CVEB / FAQ71CVEB / RZQG125L9V1B"]
["Capacitate de răcire","Nom.","","kW","","6.8","","9.5"]
["Răcire a spațiului","SEER","","","6.51","6.51","5.10","6.11","5.10"]
["","Consum anual de energie","","kWh/a","366","366","652","545","824"]
["","Capacitate","Pdesign","kW","6.80","6.80","9.50","9.50","12.00"]
["","Clasă de eficienţă energetică","","","A++","A++","B","A++","B"]
["Încălzirea spaţiului (climat temperat)","Capacitate","Pdesign","kW","6.33","6.33","11.30","10.20","12.71"]
["","SCOP/A","","","4.02","4.02","3.80","4.01","3.80"]
["","Clasă de eficienţă energetică","","","A+","A+","A","A+","A"]
["","Consum anual de energie","","kWh/a","2,205","2,205","4,164","3,562","4,683"]
["Eficienţă nominală","Consum anual de energie","","kWh","","1,000","","1,315"]
["","EER","","","","3.40","","3.62"]
["","COP","","","","3.70","","3.61"]
["","Directiva privind clasificarea energetică","Răcire","","","A","","A"]
["","","Încălzire","","","A","","A"]
["Capacitate de încălzire","Nom.","","kW","","7.5","","10.8"]
["Note","","","","","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE","","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE"]
["","","","","","(2) - Eficienţă nominală: răcire la o sarcină nominală de 35°/27°, încălzire la o sarcină nominală de 7°/20°","","(2) - Eficienţă nominală: răcire la o sarcină nominală de 35°/27°, încălzire la o sarcină nominală de 7°/20°"]