{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":9,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A"]
[]
[]
[]
[]
["","","","","","FBA35A2VEB","FBA50A2VEB","FBA60A2VEB","FBA71A2VEB"]
["Nivelul de presiune sonoră","Încălzire","","Înalt","dBA","37.0","37.0","31.0","31.0"]
["","","","Medie","dBA","34.0","34.0","28.0","28.0"]
["","","","Scăzut","dBA","29.0","29.0","25.0","25.0"]
["","Răcire","","Medie","dBA","32.0","32.0","28.0","28.0"]
["","","","Scăzut","dBA","29.0","29.0","25.0","25.0"]
["","","","Înalt","dBA","35.0","35.0","30.0","30.0"]
["Accesorii standard","Manual de utilizare","","","","1","1","1","1"]
["","Manual de instalare","","","","1","1","1","1"]
["","Furtun de drenare","","","","1","1","1","1"]
["","Clemă de metal pentru furtunul de drenare","","","","1","1","1","1"]
["","Şaibă pentru consola suportului","","","","8","8","8","8"]
["","Şuruburi","","","","40","40","40","40"]
["","Izolaţie pentru montaj","","","","2","2","2","2"]
["","Garnituri de etanşare","","","","5","5","5","5"]
["","Cleme","","","","4","4","4","4"]
["Sisteme de control","Wired remote control","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["","Infrared remote control","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["Piping connections","Lichid","","Dext","mm","6.35","6.35","6.35","9.52"]
["","Gaz","","Dext","mm","9.52","12.70","12.70","15.90"]
["","Drain","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Nivel de putere sonoră","Răcire","","","dBA","60","60","56","56"]
["Dimensiuni","Unitate","","Lățime","mm","700","700","1,000","1,000"]
["","","","Adâncime","mm","800","800","800","800"]
["","","","Înălțime","mm","245","245","245","245"]
["Carcasă","Material","","","","Tablă din oţel galvanizat","Tablă din oţel galvanizat","Tablă din oţel galvanizat","Tablă din oţel galvanizat"]
["","Colour","","","","Nevopsit (galvanizat)","Nevopsit (galvanizat)","Nevopsit (galvanizat)","Nevopsit (galvanizat)"]
["Greutate","Unitate","","","kg","28.0","28.0","35.0","35.0"]
["Ventilator","Presiune statică externă","","Ridicată","Pa","150","150","150","150"]
["","","","Nom.","Pa","30","30","30","30"]
["","Debit de aer","Încălzire","Înalt","m³/min","15.0","15.0","18.0","18.0"]
["","","","Scăzut","m³/min","10.5","10.5","12.5","12.5"]
["","","","Medie","m³/min","12.5","12.5","15.0","15.0"]
["","","Răcire","Scăzut","m³/min","10.5","10.5","12.5","12.5"]
["","","","Medie","m³/min","12.5","12.5","15.0","15.0"]
["","","","Înalt","m³/min","15.0","15.0","18.0","18.0"]
["Înălțime de drenare","mm","","","","625","625","625","625"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Frecvenţă","","","Hz","50/60","50/60","50/60","50/60"]
["","Tensiune","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Note","","","","","(1) - Nivelul de putere sonoră este o valoare absolută, care indică puterea generată de o sursă de sunet.","(1) - Nivelul de putere sonoră este o valoare absolută, care indică puterea generată de o sursă de sunet.","(1) - Nivelul de putere sonoră este o valoare absolută, care indică puterea generată de o sursă de sunet.","(1) - Nivelul de putere sonoră este o valoare absolută, care indică puterea generată de o sursă de sunet."]
["","","","","","(2) - Vezi desenele separate pentru datele electrice","(2) - Vezi desenele separate pentru datele electrice","(2) - Vezi desenele separate pentru datele electrice","(2) - Vezi desenele separate pentru datele electrice"]