{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":12,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-C8 / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FBQ100C8VEB / RZQSG100L8Y1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQSG100L8Y1B","FBQ50C8VEB / FBQ50C8VEB / RZQSG100L8Y1B","FBQ50C8VEB / FBQ50C8VEB / FBQ50C8VEB / RZQSG125L8Y1B","FBQ125C8VEB / RZQSG125L8Y1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQSG125L8Y1B","FBQ60C8VEB / FBQ60C8VEB / RZQSG125L8Y1B","FBQ140C8VEB / RZQSG140L7Y1B"]
["Capacitate de răcire","Nom.","","kW","9.5","","","","12.0","","","13.4"]
["Răcirea spaţiului","SEER","","","5.5","5.1","5.1","4.8","5.2","4.8","4.8"]
["","Consum anual de energie","","kWh/a","605","652","652","875","808","875","875"]
["","Capacitate","Pdesign","kW","9.5","9.5","9.5","12","12","12","12"]
["","Clasă de eficienţă energetică","","","A","B","B","B","A","B","B"]
["Încălzirea spaţiului (climat temperat)","Capacitate","Pdesign","kW","7.6","7.6","7.6","7.6","7.6","7.6","7.6"]
["","SCOP/A","","","4.01","3.8","3.8","3.8","3.9","3.8","3.8"]
["","Clasă de eficienţă energetică","","","A+","A","A","A","A","A","A"]
["","Consum anual de energie","","kWh/a","2,654","2,800","2,800","2,800","2,729","2,800","2,800"]
["Eficienţă nominală","Annual energy consumption","","kWh","1,435","","","","1,870","","","2,220"]
["","EER","","","3.31","","","","3.21","","","3.02"]
["","COP","","","3.65","","","","3.51","","","3.41"]
["","Directiva privind clasificarea energetică","Răcire","","A","","","","A"]
["","","Încălzire","","A","","","","B"]
["Capacitate de încălzire","Nom.","","kW","10.8","","","","13.5","","","15.5"]
["Note","","","","","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE","","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE"]
["","","","","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE","","","","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE","","","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE"]
["","","","","(2) - Eficienţă nominală: răcire la o sarcină nominală de 35°/27°, încălzire la o sarcină nominală de 7°/20°","","","","(2) - Eficienţă nominală: răcire la o sarcină nominală de 35°/27°, încălzire la o sarcină nominală de 7°/20°","","","(2) - Eficienţă nominală: răcire la o sarcină nominală de 35°/27°, încălzire la o sarcină nominală de 7°/20°"]