{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":12,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-D / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FBQ100D2VEB / RZQSG100L8Y1B","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQSG100L8Y1B","FBQ50D2VEB / FBQ50D2VEB / RZQSG100L8Y1B","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQSG125L8Y1B","FBQ50D2VEB / FBQ50D2VEB / FBQ50D2VEB / RZQSG125L8Y1B","FBQ60D2VEB / FBQ60D2VEB / RZQSG125L8Y1B","FBQ125D2VEB / RZQSG125L8Y1B","FBQ140D2VEB / RZQSG140L7Y1B"]
["Capacitate de răcire","Nom.","","kW","9.5 (2)","","","","","","12.0 (2)","13.4 (2)"]
["Răcire a spațiului","SEER","","","5.61","5.10","5.10","4.80","4.80","4.80","5.47"]
["","Consum anual de energie","","kWh/a","593","652","652","875","875","875","768"]
["","Capacitate","Pdesign","kW","9.50","9.50","9.50","12.00","12.00","12.00","12.00"]
["","Clasă de eficienţă energetică","","","A+","A","A","B","B","B","A"]
["Încălzirea spaţiului (climat temperat)","Capacitate","Pdesign","kW","7.60","7.60","7.60","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","4.15","3.80","3.80","3.80","3.80","3.80","4.01"]
["","Clasă de eficienţă energetică","","","A+","A","A","A","A","A","A+"]
["","Consum anual de energie","","kWh/a","2,564","2,800","2,800","2,800","2,800","2,800","2,653"]
["Eficienţă nominală","Consum anual de energie","","kWh","1,418","","","","","","1,858"]
["","EER","","","3.35 (1)","","","","","","3.23 (1)","3.06 (1)"]
["","COP","","","3.67 (1)","","","","","","3.63 (1)","3.40 (1)"]
["","Directiva privind clasificarea energetică","Răcire","","A","","","","","","A"]
["","","Încălzire","","A","","","","","","A"]
["Capacitate de încălzire","Nom.","","kW","10.80 (2)","","","","","","13.50 (2)","15.50 (2)"]
["Note","","","","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE","","","","","","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE"]
["","","","","(2) - Eficienţă nominală: răcire la o sarcină nominală de 35°/27°, încălzire la o sarcină nominală de 7°/20°","","","","","","(2) - Eficienţă nominală: răcire la o sarcină nominală de 35°/27°, încălzire la o sarcină nominală de 7°/20°","(2) - Eficienţă nominală: răcire la o sarcină nominală de 35°/27°, încălzire la o sarcină nominală de 7°/20°"]
["","","","","(3) - Consumul anual de energie este în conformitate cu Directiva 2002/31/CE privind etichetarea consumului de energie","","","","","","(3) - Consumul anual de energie este în conformitate cu Directiva 2002/31/CE privind etichetarea consumului de energie"]
["","","","","(4) - SEER şi SCOP sunt în conformitate cu EN 14825","","","","","","(4) - SEER şi SCOP sunt în conformitate cu EN 14825"]
["","","","","","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE"]