{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":22,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAG100BVEB / RZQG100L8Y1B","FCAG125BVEB / RZQG125L8Y1B","FCAG140BVEB / RZQG100L8Y1B","FCAG140BVEB / RZQG125L8Y1B","FCAG71BVEB / FCAG71BVEB / RZQG100L8Y1B","FCAG71BVEB / FCAG71BVEB / RZQG125L8Y1B","FCAG50BVEB / FCAG50BVEB / FCAG50BVEB / RZQG100L8Y1B","FCAG50BVEB / FCAG50BVEB / FCAG50BVEB / RZQG125L8Y1B","FCAG50BVEB / FCAG50BVEB / RZQG100L8Y1B","FCAG60BVEB / FCAG60BVEB / RZQG125L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG100L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG125L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG100L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG71L8Y1B","FCAG100BVEB / RZQG71L8Y1B","FCAG71BVEB / RZQG71L8Y1B","FCAG50BVEB / FCAG50BVEB / RZQG71L8Y1B","FCAG140BVEB / RZQG140L7Y1B"]
["Domeniu de eficiență energetică","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Capacitate de răcire","Nom.","","kW","","","","","","","","","","","","","","6.80","6.80","6.80","6.80","13.40"]
["Eficienţă nominală","EER","","","","","","","","","","","","","","","","3.30","3.39","3.39","3.30","2.50"]
["Răcire a spaţiului","Clasă de eficienţă energetică","","","","","","","","","","","","","","","","A","A++","A++","A"]
["","Capacitate","Pdesign","kW","","","","","","","","","","","","","","6.80","6.80","6.80","6.80","13.40"]
["","SEER","","","","","","","","","","","","","","","","5.10","6.80","6.72","5.10","6.44"]
["","Consum anual de energie","","kWh/a","","","","","","","","","","","","","","467","350","355","467","1,249"]
["Încălzirea spaţiului (climat temperat)","Clasă de eficienţă energetică","","","","","","","","","","","","","","","","A","A+","A+","A"]
["","Capacitate","Pdesign","kW","","","","","","","","","","","","","","6.00","6.33","6.33","6.00","11.56"]
["","SCOP/A","","","","","","","","","","","","","","","","3.80","4.20","4.20","3.80","4.27"]
["","Consum anual de energie","","kWh/a","","","","","","","","","","","","","","2,211","2,110","2,110","2,211","3,795"]
["Note","","","","","","","","","","","","","","","","","(1) - Vezi desenele separate pentru domeniul de funcţionare","(1) - Vezi desenele separate pentru domeniul de funcţionare","(1) - Capacităţile nominale de răcire se bazează pe: temperatură interioară: 27 °CDB, 19 °CWB, temperatură exterioară: 35 °CDB, lungime echivalentă traseu agent frigorific: 5 m, diferenţă de nivel: 0 m.","(1) - Vezi desenele separate pentru domeniul de funcţionare","(1) - Capacităţile nominale de răcire se bazează pe: temperatură interioară: 27 °CDB, 19 °CWB, temperatură exterioară: 35 °CDB, lungime echivalentă traseu agent frigorific: 5 m, diferenţă de nivel: 0 m."]
["","","","","","","","","","","","","","","","","","(2) - Vezi desenele separate pentru datele electrice","(2) - Vezi desenele separate pentru datele electrice","(2) - Capacităţile nominale de încălzire se bazează pe: temperatură interioară: 20°C termometru uscat, temperatura exterioară: 7°C termometru uscat, 6°C termometru umed, lungime echivalentă traseu agent frigorific: 5 m, diferenţă de nivel: 0 m.","(2) - Vezi desenele separate pentru datele electrice","(2) - Capacităţile nominale de încălzire se bazează pe: temperatură interioară: 20°C termometru uscat, temperatura exterioară: 7°C termometru uscat, 6°C termometru umed, lungime echivalentă traseu agent frigorific: 5 m, diferenţă de nivel: 0 m."]
["Capacitate de încălzire","Nom.","","kW","","","","","","","","","","","","","","","","7.50","","15.50"]
["Eficienţă nominală","COP","","","","","","","","","","","","","","","","","","3.97","","3.61"]
["","Consum anual de energie","","kWh","","","","","","","","","","","","","","","","1,003"]
["","Directiva privind clasificarea energetică","Răcire","","","","","","","","","","","","","","","","","A"]
["","","Încălzire","","","","","","","","","","","","","","","","","A"]
["Note","","","","","","","","","","","","","","","","","","","(3) - Vezi desenele separate pentru domeniul de funcţionare","","(3) - Vezi desenele separate pentru domeniul de funcţionare"]
["","","","","","","","","","","","","","","","","","","","(4) - Vezi desenele separate pentru datele electrice","","(4) - Vezi desenele separate pentru datele electrice"]