{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":13,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-G / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAHG100GVEB / RZQG100L8Y1B","FCAHG125GVEB / RZQG125L8Y1B","FCAHG140GVEB / RZQG100L8Y1B","FCAHG140GVEB / RZQG125L8Y1B","FCAHG100GVEB / RZQG71L8Y1B","FCAHG71GVEB / RZQG71L8Y1B","FCAHG71GVEB / FCAHG71GVEB / RZQG100L8Y1B","FCAHG71GVEB / FCAHG71GVEB / RZQG125L8Y1B","FCAHG140GVEB / RZQG140L7Y1B"]
["Capacitate de răcire","Nom.","","kW","","","","","","6.80 (1)","","","13.4 (1)"]
["Răcirea spaţiului","SEER","","","","","","","6.91","6.91","","","6.75"]
["","ηs,c","","%","","","","","","","","","266.9"]
["","Consum anual de energie","","kWh/a","","","","","345","345","","","1,191"]
["","Capacitate","Pdesign","kW","","","","","6.80","6.80","","","13.4"]
["","Clasă de eficienţă energetică","","","","","","","A++","A++"]
["Încălzirea spaţiului (climat temperat)","Capacitate","Pdesign","kW","","","","","7.60","7.60","","","11.8"]
["","SCOP/A","","","","","","","4.54","4.54","","","4.38"]
["","Clasă de eficienţă energetică","","","","","","","A+","A+"]
["","Consum anual de energie","","kWh/a","","","","","2,344","2,344","","","3,766"]
["","ηs,h","","%","","","","","","","","","172.1"]
["Eficienţă nominală","Consum anual de energie","","kWh","","","","","","830"]
["","EER","","","","","","","","4.09 (3)","","","3.18 (3)"]
["","COP","","","","","","","","4.80 (3)","","","4.12 (3)"]
["","Directiva privind clasificarea energetică","Răcire","","","","","","","A"]
["","","Încălzire","","","","","","","A"]
["Capacitate de încălzire","Nom.","","kW","","","","","","7.50 (2)","","","15.5 (2)"]
["Domeniu de eficiență energetică","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","","","A+++ ~ D","A+++ ~ D"]
["Note","","","","","","","","","(1) - Răcire: temperatură interioară: 27°C termometru uscat, 19°C termometru umed; temperatură exterioară: 35 °C termometru uscat; lungime tubulatură echivalentă: 7,5 m; diferenţă de nivel: 0 m","","","(1) - Răcire: temperatură interioară: 27°C termometru uscat, 19°C termometru umed; temperatură exterioară: 35 °C termometru uscat; lungime tubulatură echivalentă: 7,5 m; diferenţă de nivel: 0 m"]
["","","","","","","","","","(2) - Încălzire: temperatură interioară: 20°C termometru uscat; temperatură exterioară: 7°C termometru uscat, 6°C termometru umed; lungime echivalentă traseu agent frigorific: 7,5 m; diferenţă de nivel: 0 m","","","(2) - Încălzire: temperatură interioară: 20°C termometru uscat; temperatură exterioară: 7°C termometru uscat, 6°C termometru umed; lungime echivalentă traseu agent frigorific: 7,5 m; diferenţă de nivel: 0 m"]
["","","","","","","","","","(3) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE","","","(3) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE"]
["Outdoor unit","","","","","","","","","","RZQG100L8Y1","RZQG125L8Y1"]
["Răcirea spaţiului","Clasă de eficienţă energetică","","","","","","","","","A","A"]
["","Capacitate","Pdesign","kW","","","","","","","9.50","12.0"]
["","SEER","","","","","","","","","5.10","5.10"]
["","Consum anual de energie","","kWh/a","","","","","","","652","824"]
["Încălzirea spaţiului (climat temperat)","Clasă de eficienţă energetică","","","","","","","","","A","A"]
["","Capacitate","Pdesign","kW","","","","","","","11.30","12.71"]
["","SCOP/A","","","","","","","","","3.80","3.80"]
["","Pdh Capacitate de încălzire la -10 °","","kW","","","","","","","9.66","11.4"]
["","Consum anual de energie","","kWh/a","","","","","","","4164","4683"]