{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":14,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCQG100FVEB / RZQG71L8Y1B","FCQG35FVEB / FCQG35FVEB / RZQG71L8Y1B","FCQG71FVEB / RZQG71L8Y1B","FCQG140FVEB / RZQG100L8Y1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQG100L8Y1B","FCQG71FVEB / FCQG71FVEB / RZQG100L8Y1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG100L8Y1B","FCQG71FVEB / FCQG71FVEB / RZQG125L8Y1B","FCQG140FVEB / RZQG125L8Y1B","FCQG140FVEB / RZQG140L7Y1B"]
["Capacitate de răcire","Nom.","","kW","","","6.8","","","","","","","13.4"]
["Răcirea spaţiului","SEER","","","6.80","5.1","6.72","6.80","5.10","5.10","5.10","5.10","6.00"]
["","Consum anual de energie","","kWh/a","350","467","355","489","652","652","652","824","700"]
["","Capacitate","Pdesign","kW","6.80","6.8","6.80","9.50","9.50","9.50","9.50","12.00","12.00"]
["","Clasă de eficienţă energetică","","","A++","B","A++","A++","B","B","B","B","A+"]
["Încălzirea spaţiului (climat temperat)","Capacitate","Pdesign","kW","6.33","6","6.33","11.30","11.30","11.30","11.30","12.71","12.66"]
["","SCOP/A","","","4.20","3.8","4.20","4.61","3.80","3.80","3.80","3.80","4.10"]
["","Clasă de eficienţă energetică","","","A+","A","A+","A++","A","A","A","A","A+"]
["","Consum anual de energie","","kWh/a","2,110","2,211","2,110","3,432","4,164","4,164","4,164","4,683","4,323"]
["Eficienţă nominală","Consum anual de energie","","kWh","","","1,005"]
["","EER","","","","","3.39","","","","","","","3.21"]
["","COP","","","","","3.97","","","","","","","3.61"]
["","Directiva privind clasificarea energetică","Răcire","","","","A"]
["","","Încălzire","","","","A"]
["Capacitate de încălzire","Nom.","","kW","","","7.5","","","","","","","15.5"]
["Note","","","","","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE"]
["","","","","","","(1) - Consumul anual de energie este în conformitate cu Directiva 2002/31/CE privind etichetarea consumului de energie","","","","","","","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE"]
["","","","","","","(2) - SEER şi SCOP sunt în conformitate cu EN 14825","","","","","","","(2) - Eficienţă nominală: răcire la o sarcină nominală de 35°/27°, încălzire la o sarcină nominală de 7°/20°"]