{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":67,"n_cols":8,"rows_kept":67,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A"]
[]
[]
[]
[]
["","","","","","FDA125A5VEB","FDA200AXVEB","FDA250AXVEB"]
["Capacitate de răcire","Capacitate totală","","Nom.","kW","12.10","19.00","22.00"]
["Capacitate de încălzire","Capacitate totală","","Nom.","kW","13.50","22.4","24.0"]
["Carcasă","Colour","","","","Nevopsit","Nevopsit","Nevopsit"]
["","Material","","","","Oţel galvanizat","Tablă din oţel galvanizat","Tablă din oţel galvanizat"]
["Dimensiuni","Unitate","","Înălțime","mm","300","470","470"]
["","","","Lățime","mm","1,400","1,490","1,490"]
["","","","Adâncime","mm","700","1,100","1,100"]
["Greutate","Unitate","","","kg","45","104","115"]
["Gol în tavan necesar >","mm","","","","350"]
["Ventilator","Debit de aer","Răcire","Înalt","m³/min","39.0","64.0","69.0"]
["","","","Medie","m³/min","","50","56"]
["","","","Scăzut","m³/min","28.0","36.0","43.0"]
["","","Încălzire","Înalt","m³/min","39.0","64.0","69.0"]
["","","","Medie","m³/min","","50.0","56.0"]
["","","","Scăzut","m³/min","28.0","36.0","43.0"]
["","Presiune statică externă","","Ridicată","Pa","200","250","250"]
["","","","Nom.","Pa","50","62","62"]
["Nivel de putere sonoră","Răcire","","","dBA","66","69.0","71.0"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","40","43.0","44.0"]
["","","","Medie","dBA","","39.0","40.0"]
["","","","Scăzut","dBA","33","36.0","37.0"]
["","Încălzire","","Înalt","dBA","40","43.0","44.0"]
["","","","Medie","dBA","","39.0","40.0"]
["","","","Scăzut","dBA","33","36.0","37.0"]
["Racorduri ţevi","Lichid","","Dext","mm","9.52","9.52","9.52"]
["","Gaz","","Dext","mm","15.90","19.1","22.2"]
["","Drain","","","","VP25 (I.D. 25/O.D. 32)","BSP1","BSP1"]
["Înălțime de drenare","mm","","","","625"]
["Panou decorativ","Model","","","","BYBS125DJW1"]
["","Culoare","","","","Alb (10Y9/0,5)"]
["","Dimensiuni","","Înălțime","mm","55"]
["","","","Lățime","mm","1,500"]
["","","","Adâncime","mm","500"]
["","Greutate","","","kg","6.5"]
["Sisteme de control","Infrared remote control","","","","BRC4C65, BRC4C66"]
["","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Accesorii standard","Şuruburi","","","","16","2","2"]
["","Şaibă","","","","8","12","12"]
["","Bandă furtun","","","","1"]
["","Furtun de drenare","","","","1"]
["","Măsuri generale privind siguranţa","","","","1","1","1"]
["","Manual de instalare şi utilizare","","","","1","1","1"]
["","Cablu pentru alimentarea electrică comună","","","","2"]
["","Material de etanșare (furtun de condens)","","","","1"]
["","Material de etanşare","","","","2"]
["","Tub cu izolaţie termică (lichid)","","","","1"]
["","Tub cu izolaţie termică (gaz)","","","","1"]
["Power supply","Nume","","","","","VE","VE"]
["","Phase","","","","1~","1~","1~"]
["","Frecvenţă","","","Hz","50/60","50/60","50/60"]
["","Tensiune","","","V","220-240/220","220-240/220","220-240/220"]
["Note","","","","","(1) - Vezi desenele separate pentru datele electrice"]
["Accesorii standard","Manual de utilizare","","","","","1","1"]
["","Manual de instalare","","","","","1","1"]
["","Ţeavă de conectare gaz","","","","","1","1"]
["","Material pentru agrafe din sârmă","","","","","1","1"]
["","Șaibă arc","","","","","2","2"]
["","Şurub + şaibă","","","","","45","45"]
["","Șurub cu cap hexagonal și șaibă","","","","","49","49"]
["","Șurub cu cap hexagonal","","","","","2","2"]
["","Șaibă simplă","","","","","8","8"]