{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDBQ-B"]
[]
[]
[]
[]
["","","","","","FDBQ25B5V1","FDBQ25B8V1"]
["Nivel al presiunii sonore","Încălzire","","Înalt","dBA","35.0","35.0"]
["","","","Scăzut","dBA","29.0","29.0"]
["","Răcire","","Scăzut","dBA","28.0","28.0"]
["","","","Înalt","dBA","35.0","35.0"]
["Accesorii standard","Manual de instalare şi utilizare","","","","1","1"]
["","Filtru de aer de aspiraţie","","","","1","1"]
["Control systems","Wired remote control","","","","BRC1D52, BRC1E52A/B"]
["Racorduri conducte","Lichid","","Dext","mm","6.35"]
["","Gaz","","Dext","mm","9.52"]
["","Drain","","","","27.2"]
["Nivel de putere sonoră","Răcire","","","dBA","55","55"]
["","Încălzire","","","dBA","55","55"]
["Dimensiuni","Unitate","","Lățime","mm","652","652"]
["","","","Adâncime","mm","502","502"]
["","","","Înălțime","mm","230","230"]
["Carcasă","Material","","","","Oţel cu conţinut scăzut de carbon, zincat","Oţel cu conţinut scăzut de carbon, zincat"]
["Greutate","Unitate","","","kg","17.0","17.0"]
["Ventilator","Debit de aer","Încălzire","Înalt","m³/min","","6.95"]
["","","","Scăzut","m³/min","","5.20"]
["","","Răcire","Scăzut","m³/min","","5.20"]
["","","","Înalt","m³/min","","6.50"]
["Power supply","Phase","","","","1~","1~"]
["","Frecvenţă","","","Hz","50","50"]
["","Nume","","","","V1","V1"]
["","Tensiune","","","V","230","230 +/-10%"]
["Note","","","","","(1) - Valorile sonore sunt măsurate într-o cameră cu semiecou.","(1) - Valorile sonore sunt măsurate într-o cameră cu semiecou."]
["","","","","","(2) - Nivelul de presiune sonoră este o valoare relativă, dependentă de distanţă şi de mediul acustic. Pentru mai multe detalii, vă rugăm să consultaţi diagramele de nivel sonor.","(2) - Nivelul de presiune sonoră este o valoare relativă, dependentă de distanţă şi de mediul acustic. Pentru mai multe detalii, vă rugăm să consultaţi diagramele de nivel sonor."]
["","","","","","(3) - Nivelul de putere sonoră este o valoare absolută, care indică puterea generată de o sursă de sunet.","(3) - Nivelul de putere sonoră este o valoare absolută, care indică puterea generată de o sursă de sunet."]
["Racorduri conducte","Lichid","","Dext","mm","","6.35"]
["","Gaz","","Dext","mm","","9.52"]
["","Drain","","","","","27.2"]