{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B / RR-BW1"]
[]
[]
[]
[]
["","","","","FDQ125B8V3B9/RR125B8W1B"]
["Cooling capacity","Nom.","","kW","12.5 (1)"]
["Racorduri ţevi","Lichid","Dext","mm","9.52"]
["","Gaz","Dext","mm","15.9"]
["","Drenare","Dext","mm","26"]
["Eficienţă nominală","Annual energy consumption","","kWh","2,395"]
["","EER","","","2.61"]
["","Directiva privind clasificarea energetică","Răcire","","D"]
["Note","","","","(1) - Răcire: temperatură interioară: 27°C termometru uscat, 19°C termometru umed; temperatură exterioară: 35 °C termometru uscat; lungime tubulatură echivalentă: 7,5 m; diferenţă de nivel: 0 m"]
["","","","","(2) - Eficienţă nominală: răcire la o sarcină nominală de 35°/27°, încălzire la o sarcină nominală de 7°/20°"]