{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B / RZQ-BW1"]
[]
[]
[]
[]
["","","","","FDQ125B8V3B9 / RZQ125B8W1B"]
["Capacitate de răcire","Nom.","","kW","12.50 (1)"]
["Racorduri conducte","Lichid","Dext","mm","9.52"]
["","Gaz","Dext","mm","15.9"]
["","Drain","OD","mm","26"]
["Eficienţă nominală","Consum anual de energie","","kWh","2,075"]
["","EER","","","3.01"]
["","COP","","","3.79"]
["","Directiva privind clasificarea energetică","Răcire","","B"]
["","","Încălzire","","A"]
["Capacitate de încălzire","Nom.","","kW","14.00 (2)"]
["Note","","","","(1) - Răcire: temperatură interioară: 27°C termometru uscat, 19°C termometru umed; temperatură exterioară: 35 °C termometru uscat; lungime tubulatură echivalentă: 7,5 m; diferenţă de nivel: 0 m"]
["","","","","(2) - Încălzire: temperatură interioară: 20°C termometru uscat; temperatură exterioară: 7°C termometru uscat, 6°C termometru umed; lungime echivalentă traseu agent frigorific: 7,5 m; diferenţă de nivel: 0 m"]
["","","","","(3) - Eficienţă nominală: răcire la o sarcină nominală de 35°/27°, încălzire la o sarcină nominală de 7°/20°"]