{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C / RZQSG-L(3/8)V1"]
[]
[]
[]
[]
["","","","","FDQ125C7VEB / RZQSG125L8V1B"]
["Capacitate de răcire","Nom.","","kW","12.0"]
["Răcirea spaţiului","SEER","","","5.20"]
["","Consum anual de energie","","kWh/a","807.692"]
["","Capacitate","Pdesign","kW","12.00"]
["","Clasă de eficienţă energetică","","","A"]
["Încălzirea spaţiului (climat temperat)","Capacitate","Pdesign","kW","7.60"]
["","SCOP/A","","","3.90"]
["","Clasă de eficienţă energetică","","","A"]
["","Consum anual de energie","","kWh/a","2,728.205"]
["Eficienţă nominală","Consum anual de energie","","kWh","1,870"]
["","EER","","","3.21"]
["","COP","","","3.51"]
["","Directiva privind clasificarea energetică","Răcire","","A"]
["","","Încălzire","","B"]
["Capacitate de încălzire","Nom.","","kW","13.5"]
["Note","","","","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE"]
["","","","","(2) - Eficienţă nominală: răcire la o sarcină nominală de 35°/27°, încălzire la o sarcină nominală de 7°/20°"]