{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":9,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B9","FDXM35F3V1B9","FDXM50F3V1B9","FDXM60F3V1B9"]
["Nivelul de presiune sonoră","Încălzire","","Înalt","dBA","35.0","35.0","","38.0"]
["","","","Medie","dBA","33.0","33.0","","35.0"]
["","","","Scăzut","dBA","27.0","27.0","","30.0"]
["","Răcire","","Medium","dBA","33.0","33.0","","35.0"]
["","","","Scăzut","dBA","27.0","27.0","","30.0"]
["","","","Înalt","dBA","35.0","35.0","","38.0"]
["Accesorii standard","Manual de instalare","","","","1","1","","1"]
["","Manual de utilizare","","","","1","1","","1"]
["","Izolaţie pentru montaj","","","","1","1","","1"]
["","Plăcuţă de etanşare","","","","1","1","","1"]
["","Clemă metalică","","","","1","1","","1"]
["","Furtun de drenare","","","","1","1","","1"]
["","Şaibă pentru consola suportului","","","","8","8","","8"]
["","Material de etanşare","","","","2","2","","2"]
["","Cleme","","","","6","6","","6"]
["","Placă fixare şaibă","","","","4","4","","4"]
["","Şuruburi pentru flanşele tubulaturii","","","","1","1","","1"]
["","Filtru de aer","","","","1","1","","1"]
["Racorduri conducte","Lichid","","Dext","mm","6.35","6.35","","6.35"]
["","Gaz","","Dext","mm","9.50","9.50","","12.70"]
["","Drenare","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","","VP20 (I.D. 20/O.D. 26)"]
["Putere intrare","Răcire","","Nom.","kW","0.036","0.036","","0.060"]
["","Încălzire","","Nom.","kW","0.036","0.036","","0.060"]
["Sound power level","Răcire","","","dBA","53.0","53.0","","56.0"]
["","Încălzire","","","dBA","53.0","53.0","","56.0"]
["Dimensiuni","Unitate","","Lățime","mm","750","750","","1,150"]
["","","","Adâncime","mm","620","620","","620"]
["","","","Înălțime","mm","200","200","","200"]
["Greutate","Unitate","","","kg","21","21","","28"]
["Ventilator","Presiune statică externă","","Nom.","Pa","30","30","","40"]
["","Debit de aer","Încălzire","Înalt","m³/min","8.7","8.7","","16.0"]
["","","","Medium","m³/min","8.0","8.0","","14.8"]
["","","","Scăzut","m³/min","7.3","7.3","","13.5"]
["","","Răcire","Scăzut","m³/min","7.3","7.3","","13.5"]
["","","","Medium","m³/min","8.0","8.0","","14.8"]
["","","","Înalt","m³/min","8.7","8.7","","16.0"]
["Power supply","Fază","","","","1~","1~","","1~"]
["","Frecvenţă","","","Hz","50","50","","50"]
["","Tensiune","","","V","220-240","220-240","","220-240"]
["Note","","","","","(1) - Vezi desenele separate pentru datele electrice","(1) - Vezi desenele separate pentru datele electrice","","(1) - Vezi desenele separate pentru datele electrice"]
["Putere intrare","Răcire","","Nom.","kW","","","0.060"]
["","Încălzire","","Nom.","kW","","","0.060"]
["Dimensiuni","Unitate","","Înălțime","mm","","","200"]
["","","","Lățime","mm","","","1150"]
["","","","Adâncime","mm","","","620"]
["Greutate","Unitate","","","kg","","","28"]
["Ventilator","Debit de aer","Răcire","Înalt","m³/min","","","15.8"]
["","","","Medie","m³/min","","","14.6"]
["","","","Scăzut","m³/min","","","13.3"]
["","","Încălzire","Înalt","m³/min","","","15.8"]
["","","","Medie","m³/min","","","14.6"]
["","","","Scăzut","m³/min","","","13.3"]
["","Presiune statică externă","","Nom.","Pa","","","40"]
["Nivel de putere sonoră","Răcire","","","dBA","","","55.0"]
["","Încălzire","","","dBA","","","55.0"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","","","38.0"]
["Nivel de presiune sonoră","Răcire","","Medie","dBA","","","35.0"]
["Nivelul de presiune sonoră","Răcire","","Scăzut","dBA","","","30.0"]
["","Încălzire","","Înalt","dBA","","","38.0"]
["Nivel de presiune sonoră","Încălzire","","Medie","dBA","","","35.0"]
["Nivelul de presiune sonoră","Încălzire","","Scăzut","dBA","","","30.0"]
["Racorduri conducte","Lichid","","Dext","mm","","","6.35"]
["","Gaz","","Dext","mm","","","12.70"]
["","Drenare","","","","","","VP20 (I.D. 20/O.D. 26)"]
["Accesorii standard","Installation manual","","","","","","1"]
["","Washer for hanger bracket","","","","","","8"]
["","Operation manual","","","","","","1"]
["","Clamp metal","","","","","","1"]
["","Clamps","","","","","","6"]
["","Drain hose","","","","","","1"]
["","Filtru de aer","","","","","","1"]
["","Insulation for fitting","","","","","","1"]
["","Screws for duct flanges","","","","","","1"]
["","Sealing material","","","","","","2"]
["","Sealing pad","","","","","","1"]
["","Washer fixing plate","","","","","","4"]
["Alimentare electrică","Fază","","","","","","1~"]
["Alimentare curent","Frecvenţă","","","Hz","","","50"]
["","Tensiune","","","V","","","220-240"]